AMENDMENT-03
TO
TECHNICAL SPECIFICATION 

                                                   FOR 

               OFF-BASE GAS CONDITIONING SYSTEM

                 (Filter Separator Skid/Fine Filter Skid)
	PROJECT :
	CPCL GAS CONVERSION PROJECT FOR GT#1, GT#2, GT#3, GT#4, GT#5

	CUSTOMER :
	M/s CHENNAI PETROLEUM CORPORATION LIMITED (CPCL)

	CONSULTANT :
	--


Amendment-03
	Sl. No.
	Section / Part/Subsection
	Page No.
	Clause No.
	Actual Original Specification 
	Revised Clauses/Annexures of Specification as  per Amendment -03

	1. 
	Cl. No. 3.2.20 & 3.2.21 of PY 51361
	
	
	Performance of Fine Filter Skid:
Liquid removal efficiency

3 microns and larger – 100%

For Less than 3 microns – 99.8%
	The performance of fine filter is revised & shall be read as:

Liquid removal efficiency

3 microns and larger – 100%

For Less than 3 microns – 99.98%

	2. 
	MOC for Filter Separator (#600)
	
	
	-
	Housing : CS :

Filter elements : Fiber glass

Vane pack : SS 316
Bidder to consider above MOC

	3. 
	MOC for Fine Separator
	
	
	-
	Housing : SS :

Filter elements : Fiber glass with SS supports

Vane pack : SS 316
Bidder to consider above MOC


Notes:

1. Bidder to comply and meet all the requirements indicated above in conjunction with original Technical Specification and all its annexures.
2. Bidder to submit a stamped and signed copy of this Amendment & annexures enclosed with this document.
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