COMMON MATERIALS MANAGEMENT DEPARTMENT (STEEL DIVISION)

Ref: CMM/Steel/E1413015/Corrigendum-1


         Date: 18.06.21
Subject: Corrigendum-1 for Open tender notice no. CMM / Steel / E1413015 for procurement of various sizes of Carbon steel plates as per ASTM A 516 Gr. 60.
Charpy V-notch impact test (on longitudinal specimen) requirement for plates as per ASTM A 516 Gr.60 for thicknesses above 125 mm shall be as follows,
Impact test at -460C: 14 J (min. for 1 specimen), 18 J (Min. average for 3 specimens)

Rest all terms and conditions of the enquiry shall remain same. 

(Vineet Suman)
   Manager (CMM – Steel)

