{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[[18,3,18,5],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[19,2,19,6],[21,0,24,0],[21,1,21,6],[22,1,22,6],[23,1,23,6],[24,1,24,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED, JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:  Repair work of Service road with Paver block in Township Premises of BHEL TP Jhansi"]
["Tender Enq No-TCX/TW/22/14"]
["Sl.no.","Descripition of work","% Allocation (Item-wise) ","Unit","Qty.","Rate (Rs.)","Amount (Rs.)"]
[1,"Carriage of building rubbish",1.6419150000000001E-4,"Cum",{"$f":"+ROUND(5,2)","v":5},{"$f":"+ROUND(G7/E7,2)","v":0},{"$f":"+ROUND(C7*G19,2)","v":0}]
[2,"Earth work in excavation by mechanical means (Hydraulic excavator)/manual means over areas (exceeding 30 cm in depth, 1.5 m in width as well as 10 sqm on plan) including getting out and disposal of excavated earth lead upto 50 m and lift upto 1.5 m, as directed by Engineer-in-charge. (All kinds of soil)",2.6285719999999998E-4,"Cum",{"$f":"+ROUND(5,2)","v":5},0,{"$f":"+ROUND(C8*G19,2)","v":0}]
[3,"Filling available excavated earth in (excluding rock)",5.2488499999999997E-5,"Cum",{"$f":"+ROUND(1,2)","v":1},0,{"$f":"+ROUND(C9*G19,2)","v":0}]
[4," Providing and laying in position cement concrete of specified grade excluding the cost of centering and shuttering - All work up to plinth level :\"1:2:4 (1 cement : 2 coarse sand (zone-III) : 4 graded stone aggregate 20 mm nominal size). ",2.70098953E-2,"Cum",{"$f":"+ROUND(20,2)","v":20},0,{"$f":"+ROUND(C10*G19,2)","v":0}]
[5,"Providing and laying in position cement concrete of specified grade excluding the cost of centering and shuttering - All work up to plinth level : 1:3:6 (1 Cement : 3 coarse sand (zone-III) : 6 graded stone aggregate 40 mm nominal size)",1.3527795000000001E-3,"Cum",{"$f":"+ROUND(1,2)","v":1},0,{"$f":"+ROUND(C11*G19,2)","v":0}]
[6,"Providing and laying in position specified grade of reinforced cement concrete, excluding the cost of centering, shuttering, finishing and reinforcement - All work up to plinth level : 1:1.5:3 (1 cement : 1.5 coarse sand (zone-III): 3 graded stone aggregate 20 mm nominal size)",2.8674054000000001E-3,"Cum",{"$f":"+ROUND(2,2)","v":2},0,{"$f":"+ROUND(C12*G19,2)","v":0}]
[7,"Providing and laying in position specified grade of reinforced cement concrete, excluding the cost of centering, shuttering, finishing and reinforcement - All work up to plinth level : 1:2:4 (1 cement : 2 coarse sand : 4 graded stone aggregate 20 mm  nominal size). ",2.9436235E-3,"Cum",{"$f":"+ROUND(2,2)","v":2},0,{"$f":"+ROUND(C13*G19,2)","v":0}]
[8,"Centering and shuttering including strutting, propping etc. and removal of form for all heights : Foundations, footings, bases of columns, etc. for mass concrete.",1.154581E-3,"Sqm",{"$f":"+ROUND(15,2)","v":15},0,{"$f":"+ROUND(C14*G19,2)","v":0}]
[9,"Demolishing cement concrete manually/ by mechanical means including disposal of material within 50 metres lead as per direction of Engineer - in - charge. Nominal concrete 1:3:6 or richer mix (i/c equivalent design mix) \n",8.3232079999999995E-4,"Cum",{"$f":"+ROUND(2,2)","v":2},0,{"$f":"+ROUND(C15*G19,2)","v":0}]
[10,"Demolishing R.C.C. work manually/ by mechanical means including stacking of steel bars and disposal of unserviceable material within 50 metres lead as per direction of Engineer - in- charge. ",1.8213379E-3,"Cum",{"$f":"+ROUND(3,2)","v":3},0,{"$f":"+ROUND(C16*G19,2)","v":0}]
[11,"Item not covered above but covered in DSR 2016",4.1472017000000003E-3,"LS",{"$f":"+ROUND(10000,2)","v":10000},0,{"$f":"+ROUND(C17*G19,2)","v":0}]
[12,"Providing and laying 80 mm thick factory made cement concrete interlocking paver block of M-40 grade made by block making machine with rubber molded unifier finish strong vibratory compaction, of approved size, design & shape, laid in required colour (Red, yellow, Gray) and pattern over and including 50 mm thick compacted bed of stone dust, filling the joints with fine stone dust etc. all complete as per the direction of engineer – incharge.",0.95739131779999997,"Sqm",{"$f":"+ROUND(2800,2)","v":2800},0,{"$f":"+ROUND(C18*G19,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C18)","v":1.0000000001},"Total amount quoted by bidder",null,null,0]
[null,"IN WORDS",{"$f":"rup(G19)","v":0}]
[]
["Note:","1. GST extra as applicable"]
[null,"2. Bidder has to quote in above unlocked cell (G-19) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"3. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"4.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[]
[null,null,null,null,"(Signature and Seal of  Contractor  )"]