{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[[24,3,24,5],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[25,2,25,6],[27,0,30,0],[27,1,27,6],[28,1,28,6],[29,1,29,6],[30,1,30,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:  Misc. repair and maintenance works of Hospital ward in the Township premises of BHEL TP Jhansi"]
["Tender Enq No-TCX/TW/24/03"]
["Sl.no.","Descripition of work","% Allocation (Item-wise) ","Unit","Qty.","Rate (Rs.)","Amount (Rs.)"]
[1,"P and L in position Cement concrete -1:2:4 (1 Cement: 2 coarse sand: 4 graded stone aggregate 20mm nominal size) excluding the cost of entering and shuttering all work up to plinth level.",4.9927399999999999E-3,"cum",1,{"$f":"+ROUND(G7/E7,2)","v":0},{"$f":"+ROUND(C7*G25,2)","v":0}]
[2,"Brick  work  with  FPS  bricks  of    (II nd class kanpur brick ) in Super  structure 1:6 (1 cement : 6 fine sand ) upto floor five level.",1.465436E-2,"cum",2,0,{"$f":"+ROUND(C8*G25,2)","v":0}]
[3,"Providing Half Brick masonry in super structure upto floor five level . 1:4 ( 1 cement :4 coarse sand )",2.61693E-3,"sqm",3,0,{"$f":"+ROUND(C9*G25,2)","v":0}]
[4,"Providing and fixing Ist quality ceramic glazed wall tiles conforming to IS: 15622 (thickness to be specified by the manufacturer), of approved make, in all colours, shades except burgundy, bottle green, black of any size as approved by Engineer-in-Charge, in skirting, risers of steps and dados, over 12 mm thick bed of cement mortar 1:3 (1 cement : 3 coarse sand) and jointing with grey cement slurry @ 3.3kg per sqm, including pointing in white cement mixed with pigment of matching shade complete",3.3343699999999997E-2,"sqm",34,0,{"$f":"+ROUND(C10*G25,2)","v":0}]
[5,"Providing and laying Ceramic glazed floor tiles of size 300x300 mm (thickness to be specified by the  manufacturer), of 1st quality conforming to IS : 15622, of approved make, in all colours, shades, except White, Ivory, Grey, Fume Red Brown, laid on 20 mm thick bed of cement mortar 1:4 (1 Cement : 4 Coarse sand), jointing with grey cement slurry @ 3.3kg/sqm including pointing the joints with white cement and matching pigments etc.,  complete",1.4246099999999999E-2,"sqm",15,0,{"$f":"+ROUND(C11*G25,2)","v":0}]
[6,"Providing and laying Vitrified tiles in floor with different sizes (thickness to be specified by the manufacturer), with water absorption less than 0.08% and conforming to IS:15622 , of approved brand & manufacturer, in all colours and shade, laid with cement based high polymer modified quick set tile adhesive (water based) conforming to IS : 15477, in average 6 mm thickness, including grouting of joints (Payment for grouting of joints to be made separately). Size of Tile 600x600 mm",0.15555906999999999,"sqm",109,0,{"$f":"+ROUND(C12*G25,2)","v":0}]
[7,"12 mm cement plaster of mix :  1:6 (1 cement: 6 fine sand) \n",2.0908699999999999E-3,"sqm",10,0,{"$f":"+ROUND(C13*G25,2)","v":0}]
[8,"15 mm cement plaster on the rough side of single or half brick wall of mix :  1:6 (1 cement: 6 fine sand) ",2.3997300000000001E-3,"sqm",10,0,{"$f":"+ROUND(C14*G25,2)","v":0}]
[9,"Demolishing cement concrete  including disposal of material within 50 meter lead (1:3:6)",3.07705E-3,"cum",2,0,{"$f":"+ROUND(C15*G25,2)","v":0}]
[10,"Demolishing brick work in cement mortar including stacking of serviceable material and disposal of unserviceable material within 50 meter lead.",3.9012600000000001E-3,"cum",3,0,{"$f":"+ROUND(C16*G25,2)","v":0}]
[11,"Providing and layingAPP (Atactic Polypropylene Polymer) modified prefabricated five layer 3 mm thick water proofing membrane, black finished reinforced with non-woven polyester matt consisting of a coat of bitumen primer for bitumen membrane @ 0.40 litre/sqm by the same membrane manufacture of density at 25°C, 0.87-0.89 kg/ litre and viscocity 70-160 cps. Over the primer coat the layer of membrane shall be laid using Butane Torch and sealing all joints etc, and preparing the surface complete. The vital physical and chemical parameters of the membrane shall be as under : Joint strength in longitudinal and transverse direction at 23°C as 650/ 450N/5cm. Tear strength in longitudinal and transverse direction as\n300/250N. Softening point of membrane not less than 150°C. Cold flexibility shall be upto -2°C when tested in accordance with ASTM, D - 5147. The laying of membrane shall be got done through the authorised applicator of the manufacturer of membrane....3 mm thick",2.0604790000000001E-2,"sqm",36,0,{"$f":"+ROUND(C17*G25,2)","v":0}]
[12,"Providing and applying fibre reinforced elastomeric liquid water proofing membrane with resilient acrylic polymers having Sun Reflectivity Index (SRI) of 105 on top of concrete roof in three coats @10.76 litre/ 10 sqm. One coat of self-priming of elastomeric waterproofing liquid (dilution with water in the ratio of 3:1) and two coats of undiluted elastomeric waterproofing liquid (dry film thickness of complete application/ system not less than 500 microns). The operation shall be carried out after scrapping and properly cleaning the surface to remove loose particles with wire brushes, complete in all respect as per the direction of Engineer-in-Charge.",5.1011210000000001E-2,"sqm",114,0,{"$f":"+ROUND(C18*G25,2)","v":0}]
[13,"All items of DSR 2016 not covered above",4.6687319999999997E-2,"L.S.",30000,0,{"$f":"+ROUND(C19*G25,2)","v":0}]
[14,"Providing and fixing glazing in fixed aluminium structure with EPDM rubber / neoprene gasket etc. complete as per the architectural drawings and the directions of Engineer-in-charge :- With French embossed (etched) float glass panes  of 12 mm thickness.Brand- Modiguard/ SAINTGOBAIN / TRIVENI or equivalent",4.8644949999999999E-2,"Sqm",5,0,{"$f":"+ROUND(C20*G25,2)","v":0}]
[15,"Fixed frame work for aesthetic purpose with built up standard tubular sections/appropriate Z sections and other sections of Polyester powder coated aluminium with dash fasteners of required dia and size, including necessary filling up the gaps at junctions, i.e. at top, bottom and sides with required EPDM rubber/ neoprene gasket etc. Aluminium sections shall be smooth, rust free, straight, mitred and jointed mechanically wherever required including cleat angle, Aluminium snap beading for glazing / panelling, C.P. brass / stainless steel screws, all complete as per required pattern & shape and the directions of Engineer-in-charge.",4.0166029999999998E-2,"Kg",38,0,{"$f":"+ROUND(C21*G25,2)","v":0}]
[16,"Providing and fixing suspended false ceiling made out of 10 mm to 12.50 mm thick Gypsum Plaster Boards consiting of  G.I standard section framework in the pattern and design as per direction of the  Engineer-in-charge. The G.I. Section frame work shall be tied to the roof and walls with the anchor fastener screws/bolts of appropriate size recommended by the manufaturer (max. 450 mm C/C) . The boards shall be fixed to the frame work with the screws and the joints shall be flushed and finished with requisite jointing compounds paper tapes etc. Rates includes execution of works in different levels/offsets etc. The surface shall be finished evenly by applying putty,sand papering,applying 2 coat primer evenly complete. Rate inclusive of materials transportation, loading/unloading labor, tools and tackles up to any lead and lift complete in all respects. Brand- Gyproc,Armstrong,Shera or equivelant.",0.11361164,"Sqm",51,0,{"$f":"+ROUND(C22*G25,2)","v":0}]
[17,"Providing and fixing suspended false ceiling made out of minimum  7 mm thick PVC tile/ Boards consiting of  G.I standard section framework in the pattern and design as per direction of the  Engineer-in-charge. The G.I. Section frame work shall be tied to the roof and walls with the anchor fastener screws/bolts of appropriate size recommended by the manufaturer . The PVC tiles/boards shall be fixed to the frame work with the screws and the joints shall be flushed and finished with requisite jointing compounds paper tapes etc. Rates includes execution of works in different levels/offsets etc. The surface shall be finished evenly complete. Rate inclusive of materials transportation, loading/unloading labor, tools and tackles up to any lead and lift complete in all respects.",0.27862751000000002,"Sqm",95,0,{"$f":"+ROUND(C23*G25,2)","v":0}]
[18,"Providing and fixing  PVC  wall tiles minimum 5 mm thick (thickness to be specified by the manufacturer), of approved make, in all colours, shades  consiting of  accessories required in the pattern and design as per direction of the  Engineer-in-charge.The PVC  wall tiles shall be tied to the roof and walls with the anchor fastener screws/bolts as required of appropriate size recommended by the manufaturer.Rate inclusive of materials transportation, loading/unloading labor, tools and tackles up to any lead and lift complete in all respects.",0.16376473999999999,"Sqm",72,0,{"$f":"+ROUND(C24*G25,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C24)","v":1},"Total amount quoted by bidder",null,null,0]
[null,"IN WORDS",{"$f":"rup(G25)","v":0}]
[]
["Note:","1. GST extra as applicable"]
[null,"2. Bidder has to quote in above unlocked cell (G-25) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"3. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"4.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[null,null,null,null,"(Signature and Seal of  Contractor  )"]