{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[[16,3,16,5],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[17,2,17,6],[19,0,22,0],[19,1,19,6],[20,1,20,6],[21,1,21,6],[22,1,22,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:  Repair and maintenance of roof and side sheeting work in the Township premises of BHEL TP Jhansi"]
["Tender Enq No-TCX/TW/24/04"]
["Sl.no.","Descripition of work","% Allocation (Item-wise) ","Unit","Qty.","Rate (Rs.)","Amount (Rs.)"]
[1,"Earth  work  in  excavation  by mechanical  means  (Hydraulic excavator)  /  manual  means  in  foundation  trenches or drains, All kinds of soil  (not exceeding 1.5 m in width or 10 sqm on plan) including dressing of sides and ramming of bottoms, lift upto 1.5 m, including getting out the  excavated  soil  and  disposal  of  surplus excavated  soil  as directed, within a lead of 50 m. ",7.8392839999999995E-4,"cum",3,{"$f":"+ROUND(G7/E7,2)","v":0},{"$f":"+ROUND(C7*G17,2)","v":0}]
[2,"Filling available excavated earth in (excluding rock)",1.9745010000000001E-4,"cum",1,0,{"$f":"+ROUND(C8*G17,2)","v":0}]
[3,"P and L in position Cement concrete -1:2:4 (1 Cement: 4 coarse sand: 8 graded stone aggregate 20mm nominal size) excluding the cost of entering and shuttering all work up to plinth level.",1.52424181E-2,"cum",3,0,{"$f":"+ROUND(C9*G17,2)","v":0}]
[4,"P and L in position Cement concrete -1:4:8 (1 Cement: 4 coarse sand: 8 graded stone aggregate 40mm nominal size) excluding the cost of entering and shuttering all work upto plinth level.",5.0894067000000001E-3,"cum",1,0,{"$f":"+ROUND(C10*G17,2)","v":0}]
[5,"Steel work welded in builtup sections / Framed work including  cutting , hoisting , fixing in position and applying a priming coat of approved steel primer  using structural steel etc. as required in gratings , frames , guard bar, ladder, railing brackets",6.9516842600000003E-2,"kg",560,0,{"$f":"+ROUND(C11*G17,2)","v":0}]
[6,"All items of DSR 2016 but not covered above.",2.3755405E-2,"basic value",15000,0,{"$f":"+ROUND(C12*G17,2)","v":0}]
[7,"Supply and installation of coated galvalume steel sheet (Maximum height up to 30.0 m ) having maximum of pitch of 205 mm c/c and minimum 28 mm crest depth in length for roofing / side cladding as per the site requiremen. The supplied material is to be manufactured out of 0.50 mm TCT (Total coated thickness and 550 MPA tensile strength, with zinc aluminium alloy of AZ-150 (As per AS-1397:1993). The sheet shall have a hot dip metallic zinc aluminium alloy coating of zinc (43%), silicon(1.5%) and aluminium (55%) with total mass coating of 150 gms/sqm considering both sides together, self drilling/ self tapping screws with EPDM seal fixed to the existing MS purlins / MS runners complete as per drawing and as directed by engineer-in-charge.",0.50866754329999997,"sqm",435,0,{"$f":"+ROUND(C13*G17,2)","v":0}]
[8,"Supply & Fixing of flashings, ridges, cappings, corner pieces etc. made of 0.5mm TCT galvolume sheet in required shape and size having a yield strength of 550 Mpa (with 150 gsm/ sqm minimum coating mass total of both side as per AZ 150), smp colour coating provided on exposed face with 20 microns thick finish and inner face provided with back-coat pre-coating of 5-7 microns & fixed with stitching screw complete.",9.4301209900000002E-2,"Metre",144,0,{"$f":"+ROUND(C14*G17,2)","v":0}]
[9,"Providing and fixing fire retardant and U.V. resistant profiled and solid transparent embossed polycarbonate sheet of minimum 3 mm thick of matching profile  at the roof top of manufacturing blocks including:                          -Removal of existing old GS sheet/Galvolume sheet including removal of ridges, hips valley, gutters etc. and stacking the material with 50 meters lead. To avoid breakage of sheets, adjacent sheets may also be required to be removed / lossened and then fixed accordingly.         -Rates shall be inclusive of GI hooks, Self-tapping screws or any other material required for fixing.                         For measurement, Overlap between new and existing sheet will not be deducted and would be considered during calculation of area.Whereas, the overlap arising between new sheets would be deducted during calculation of area. During dismantling, if adjacent AC sheets gets broken, it shall be provided free of cost from BHEL and the fixing and installation shall be done by contractor at his own cost.  The above item comprises of all the activities required to replace the existing sheet with FRP sheet. ",0.2101742036,"Sqm",53,0,{"$f":"+ROUND(C15*G17,2)","v":0}]
[10,"Providing and fixing fiberglass reinforced plastic sheet 2 mm thick corrugated of  matching profile  at the roof top of manufacturing blocks including:                          -Removal of existing old GS sheet/Galvolume sheet including removal of ridges, hips valley, gutters etc. and stacking the material with 50 meters lead. To avoid breakage of sheets, adjacent sheets may also be required to be removed / lossened and then fixed accordingly.         -Rates shall be inclusive of GI hooks, Self-tapping screws or any other material required for fixing.                         For measurement, Overlap between new and existing sheet will not be deducted and would be considered during calculation of area.Whereas, the overlap arising between new sheets would be deducted during calculation of area. During dismantling, if adjacent AC sheets gets broken, it shall be provided free of cost from BHEL and the fixing and installation shall be done by contractor at his own cost.  The above item comprises of all the activities required to replace the existing sheet with FRP sheet.                                      ",7.2271592499999995E-2,"Sqm",28,0,{"$f":"+ROUND(C16*G17,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C16)","v":1.0000000002},"Total amount quoted by bidder"]
[null,"IN WORDS",{"$f":"rup(G17)","v":0}]
[]
["Note:","1. GST extra as applicable"]
[null,"2. Bidder has to quote in above unlocked cell (G-17) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"3. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"4.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[null,null,null,null,"(Signature and Seal of  Contractor  )"]