{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[[25,3,25,5],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[26,2,26,6],[28,0,31,0],[28,1,28,6],[29,1,29,6],[30,1,30,6],[31,1,31,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work: Misc. repair and maintenance works of Club Bundela provided in the Township premises of BHEL TP Jhansi"]
["Tender Enq No-TCX/TW/24/05"]
["Sl.no.","Descripition of work","% Allocation (Item-wise) ","Unit","Qty.","Rate (Rs.)","Amount (Rs.)"]
["Section\"A\"  Based on DSR 2016"]
[1,"P and L in position Cement concrete -1:2:4 (1 Cement: 4 coarse sand: 8 graded stone aggregate 20mm nominal size) excluding the cost of entering and shuttering all work up to plinth level.",2.1879312682466501E-2,"cum",6,{"$f":"+ROUND(G8/E8,2)","v":0},{"$f":"+ROUND(C8*G26,2)","v":0}]
[2,"Brick  work  with  FPS  bricks  of    (II nd class kanpur brick ) in Super  structure 1:6 (1 cement : 6 fine sand ) upto floor five level.",4.2812455493639365E-2,"cum",8,0,{"$f":"+ROUND(C9*G26,2)","v":0}]
[3,"Providing Half Brick masonry in super structure upto floor five level . 1:4   ( 1 cement :4 coarse sand )",3.1855504815104601E-3,"sqm",5,0,{"$f":"+ROUND(C10*G26,2)","v":0}]
[4,"12 mm cement plaster of mix :  1:6 (1 cement: 6 fine sand) \n",4.8867606925453548E-3,"sqm",32,0,{"$f":"+ROUND(C11*G26,2)","v":0}]
[5,"15 mm cement plaster on the rough side of single or half brick wall of mix :  1:6 (1 cement: 6 fine sand) ",5.6086112929556956E-3,"sqm",32,0,{"$f":"+ROUND(C12*G26,2)","v":0}]
[6,"Demolishing cement concrete  including disposal of material within 50 meter lead (1:3:6)",1.1236947573248187E-3,"cum",1,0,{"$f":"+ROUND(C13*G26,2)","v":0}]
[7,"Demolishing brick work in cement mortar including stacking of serviceable material and disposal of unserviceable material within 50 meter lead.",1.8995792326205266E-3,"cum",2,0,{"$f":"+ROUND(C14*G26,2)","v":0}]
[8,"Providing and layingAPP (Atactic Polypropylene Polymer) modified prefabricated five layer 3 mm thick water proofing membrane, black finished reinforced with non-woven polyester matt consisting of a coat of bitumen primer for bitumen membrane @ 0.40 litre/sqm by the same membrane manufacture of density at 25°C, 0.87-0.89 kg/ litre and viscocity 70-160 cps. Over the primer coat the layer of membrane shall be laid using Butane Torch and sealing all joints etc, and preparing the surface complete. The vital physical and chemical parameters of the membrane shall be as under : Joint strength in longitudinal and transverse direction at 23°C as 650/ 450N/5cm. Tear strength in longitudinal and transverse direction as\n300/250N. Softening point of membrane not less than 150°C. Cold flexibility shall be upto -2°C when tested in accordance with ASTM, D - 5147. The laying of membrane shall be got done through the authorised applicator of the manufacturer of membrane....3 mm thick",0.18602405607345254,"sqm",445,0,{"$f":"+ROUND(C15*G26,2)","v":0}]
[9,"Providing and laying Vitrified tiles in floor with different sizes (thickness to be specified by the manufacturer), with water absorption less than 0.08% and conforming to IS:15622 , of approved brand & manufacturer, in all colours and shade, laid with cement based high polymer modified quick set tile adhesive (water based) conforming to IS : 15477, in average 6 mm thickness, including grouting of joints (Payment for grouting of joints to be made separately). Size of Tile 600x600 mm",5.5886974493571662E-2,"sqm",52,0,{"$f":"+ROUND(C16*G26,2)","v":0}]
[10,"Providing and applying plaster of paris putty of 2 mm thickness over plastered surface to prepare the surface even and smooth complete.",2.2901794472853957E-2,"sqm",190,0,{"$f":"+ROUND(C17*G26,2)","v":0}]
[11,"Finishing with Deluxe Multi surface paint system for interiors and exteriors using Primer as per manufacturers specifications :Two or more coats applied on walls @ 1.25 ltr/10 sqm over and including one coat of Special primer applied @ 0.75 ltr /10 sqm",1.627858788710736E-2,"sqm",173,0,{"$f":"+ROUND(C18*G26,2)","v":0}]
[12,"Repairs to plaster of thickness 12 mm to 20 mm in patches of area 2.5 sq. meters and under, including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete, including disposal of rubbish to the dumping ground, all complete as per directions of Engineer-In-Charge.",6.7332503315891898E-4,"sqm",3,0,{"$f":"+ROUND(C19*G26,2)","v":0}]
[13,"DSR 2016",3.4099047257755935E-2,"L.S.",30000,0,{"$f":"+ROUND(C20*G26,2)","v":0}]
["Section \"B\"Premiume Interior works (Non-DSR items )"]
[14,"Texture painting (Matellic finshed) with co-polymer emulsion based paint  for interior application to create different types of special effects such as crinkle, dapple, weaving, canvas, spatula, colourwash, ragging, sponging, combing, and brushing  etc. as per direction of Engineer-in-charge. Brand-Asian paint /Nerolac/",0.17536090803209792,"Sqm",125,0,{"$f":"+ROUND(C22*G26,2)","v":0}]
[15,"Providing and fixing pre manufactured gypsum molding / cornice corner  in required pattern and shape & size and  as per the architectural drawings and the directions of Engineer-in- charge",8.9650766913365685E-4,"Mtr.",4,0,{"$f":"+ROUND(C23*G26,2)","v":0}]
[16,"Providing and fixing suspended false ceiling made out of 10 mm to 12.50 mm thick Gypsum Plaster Boards consiting of  G.I standard section framework in the pattern and design as per direction of the  Engineer-in-charge. The G.I. Section frame work shall be tied to the roof and walls with the anchor fastener screws/bolts of appropriate size recommended by the manufaturer (max. 450 mm C/C) . The boards shall be fixed to the frame work with the screws and the joints shall be flushed and finished with requisite jointing compounds paper tapes etc. Rates includes execution of works in different levels/offsets etc. The surface shall be finished evenly by applying putty,sand papering,applying 2 coat primer evenly complete. Rate inclusive of materials transportation, loading/unloading labor, tools and tackles up to any lead and lift complete in all respects. Brand- Gyproc,Armstrong,Shera or equivelant.",0.25869803524874474,"Sqm",159,0,{"$f":"+ROUND(C24*G26,2)","v":0}]
[17,"Providing and fixing  PVC  wall tiles minimum 5 mm thick (thickness to be specified by the manufacturer), of approved make, in all colours, shades  consiting of  accessories required in the pattern and design as per direction of the  Engineer-in-charge.The PVC  wall tiles shall be tied to the roof and walls with the anchor fastener screws/bolts as required of appropriate size recommended by the manufaturer.Rate inclusive of materials transportation, loading/unloading labor, tools and tackles up to any lead and lift complete in all respects",0.16778479919906059,"Sqm",101,0,{"$f":"+ROUND(C25*G26,2)","v":0}]
[null,"Total ",{"$f":"SUM(C8:C25)","v":1},"Total amount quoted by bidder"]
[null,"IN WORDS",{"$f":"rup(G26)","v":0}]
[]
["Note:","1. GST extra as applicable"]
[null,"2. Bidder has to quote in above unlocked cell (G-26) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"3. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"4.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[null,null,null,null,"(Signature and Seal of  Contractor  )"]