{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["PRICE BID 01"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PRICE BID 01","index":0,"n_rows":34,"n_cols":9,"rows_kept":34,"cut":false,"hidden":false,"merged":[[33,3,33,4],[0,0,0,6],[2,0,2,8],[4,0,4,8],[6,2,21,2],[6,7,21,7],[6,8,21,8],[6,0,21,0],[27,1,27,8],[28,1,28,8],[23,0,23,1],[23,3,23,8],[33,5,33,6],[0,12,0,20],[6,3,21,3],[6,4,21,4],[6,5,21,5],[6,6,21,6],[1,0,1,6],[3,0,3,6]]}
["BHARAT HEAVY ELECTRICALS LIMITED,  JHANSI"]
["FACTORY CIVIL DEPARTMENT"]
["Price bid "]
["Name of Work: Soil testing work for proposed UHV lab inside factory premises in BHEL Jhansi."]
["Tender No-FCX/TW/24/01"]
["Sr. No","Description ","% Allocation (Item-wise)","Unit "," Qty","Rate ","Amount (Rs)","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Making 150 mm nominal diameter bore hole at various location upto required depth as per site condition maximum of 7 meter below ground level in all type of the soil including laterite/weathered soft rock using suitable approved method of boring including chesiling, cleaning, providing casing pipes as required or as directed for perfoming standard penetration test at every 1 m interval down to required depth (around 7 m) below ground level (starting depth 2 m from ground level) and at change of strata. Bore hole location shall be identified and shown by BHEL prior to commencement.",{"$f":"G7/50000","v":1},"Number of Bore Holes",2,25000,{"$f":"F7*E7","v":50000},{"$f":"I7/E7","v":0},{"$f":"I23*C7","v":0}]
[null,"Conducting Laboratory test on soil samples at an approved laboratory including preparation of soil samples at every 1 m interval down to required depth below ground level (starting depth 2 m from ground level) and at change of strata to determine the following properties etc. all complete as per specification."]
[null,"Atterberg limits"]
[null,"Dry and Bulk Density"]
[null,"Moisture Content"]
[null,"Maximum Dry Density and Optimum Moisture Content and formulation of Curves (OMC and MDD Curves)"]
[null,"Soil Profile and Sieve analysis"]
[null,"Specific Gravity and Void ratio "]
[null,"Direct Shear Test or Triaxial Test as applicable"]
[null,"Shrinkage Limit Test"]
[null,"Swell Pressure test "]
[null,"Net Safe Bearing Capacity using appropriate method"]
[null,"Bore Log Charts"]
[null,"Unconfined Compressive strength"]
[null,"Conducting Electrical Resistivity Test (ERT) at various locations complete as directed by the engineer- In-charge."]
[null,"Preparation and submission of draft report in one copy and final report in two hard copies and soft copy via email after the approval of draft report including all field records, laboratory test results, graphs, analysis of test results and suitable recommendation regarding type of foundation etc all complete as per specification etc."]
[null,"Total (Excluding GST) (In Rs.)",{"$f":"SUM(C7)","v":1},null,null,null,{"$f":"G7","v":50000},null,0]
["In words ",null,null,{"$f":"rup(I23)","v":0}]
[]
[]
[null,"Note -GST extra as applicable"]
[null,"1. Bidder has to quote in above unlocked cell (I-23) only. Item rate shall be calculated automatically. Calculated item rates upto four  decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected."]
[]
[]
[]
[null,null,null,"(Signature and Seal of  Contractor  )"]
[null,null,null,null,null,"Prepared By "]