{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[[11,0,11,8],[12,0,12,8],[9,2,9,8],[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8],[5,0,5,8]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["FACTORY CIVIL DEPARTMENT "]
["PRICE BID "]
["Name of work: False Ceiling  work in ADM building in BHEL Jhansi."]
[]
["Tender Enquiry No- FCX/TW/24/24"]
["Sl. No.","Description of work ","% Allocation (Item-wise)","Unit "," Quantity ","Rate ","Amount (Rs)","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Providing and fixing false ceiling at all height of specified material in true horizontal level including providing and fixing of framework made of special metal sections consisting of T-sections and L sections suitably fixed according to tile/board size and as per direction of Engineer-in-charge. The entire structure is to be designed and installed on the exiting RCC / Wall structure in such a manner that it should be able to bear its self-load as well as the load of the lighting arrangement fixed in the structure. The work includes the cost of making openings for light fittings, grills, diffusers, cut-outs made with frame of perimeter channels suitably fixed, all complete as per drawings, specification and direction of the Engineer in Charge.\n7.0 mm thick square edge PVC Laminated Gypsum Tile of size 595x595 mm, made of Gypsum plasterboard, manufactured from natural gypsum as per IS 2095 Part I and laminated with white 0.10 mm thick fire retardant PVC film on the face side and metalized polyester on the back side with all edges sealed with the face side PVC film which goes around and wraps the edges and is bonded to the edges and the back side metalized polyester film so as to make the tile a completely sealed unit.",{"$f":"G8/$G$9","v":1},"Sqm ",{"$f":"'[1]Msrment '!H18","v":1898},{"$f":"'[1]CST Budgetary'!H9","v":810},{"$f":"F8*E8","v":1537380},{"$f":"I8/E8","v":0},{"$f":"I9*C8","v":0}]
[null,"Sub Total ",null,null,null,null,{"$f":"SUM(G8:G8)","v":1537380},null,0]
[null,"Amount in words ",{"$f":"rup(I9)","v":0}]
["Note -GST extra as applicable"]
["1. Bidder has to quote in above unlocked cell (I- 9) only. Item rate shall be calculated automatically. Calculated item rates upto four  decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
["2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT, the offer of the bidder will be rejected."]
[]
[]
[]
[null,null,null,null,"Signature and seal of contractor"]
[null,null,null,null,null,"(Signature and Seal of Contractor)"]