{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["26"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"26","index":0,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8],[4,0,4,8],[12,0,12,8],[13,0,13,8],[6,0,7,0],[6,1,7,1],[6,3,7,3],[6,4,7,4],[6,5,7,5],[6,6,7,6],[9,2,9,8],[6,2,7,2],[11,0,11,8],[6,7,7,7],[6,8,7,8],[10,0,10,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["FACTORY CIVIL DEPARTMENT "]
["Price bid "]
["Name of work:  Maintaining of continuous operation of oxidation pond area located inside factory area for a period of 3 years."]
["Tender Enquiry No- FCX/TW/24/26"]
["Sl. No.","Description of work ","% Allocation (Item-wise)","Unit "," Quantity ","Rate ","Amount (Rs)","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Two oxidation ponds of sizes 78 x 33 m and 78 x 27.5 m are located side by side and only one is operation at any given time in the oxidation pond compound. The scope of work includes :-\n1.\tMaintaining of continuous operation of  oxidation pond compound by deployment on 2 workers on continuous basis. Work to be carried out with following activities-\n•\tCleaning of oxidation pond compound by way of uprooting of vegetation.\n•\tCleaning of active oxidation pond by removing algae using nets and other means.\n•\tOperation of installed submersible pumps and centrifugal pump as per direction of Engineer-in-charge.\n•\tMaintaining nursery at designated place and overall upkeep of the oxidation pond compound by using the treated water of oxidation pond. \n•\tTools and tackles for cleaning and horticulture activities shall be bought by contractor on their own cost. Existing GI pipe fitting available in the compound shall be used for distribution of water to plants. Other items like flexible pipe (as per requirement) etc. shall be bought by contractor. \n2.\tProviding and operating 2 numbers of 2 HP Submersible pumps for a period of minimum 6 hours per day to increase the oxygen content of the collected sewage in the oxidation pond by way of aeration. This item includes supply of 2 number 2 HP Submersible pumps on returnable basis and their installation at oxidation pond as directed by Engineer-in-charge. Pumps are to be operated for a minimum of 6 hours per day and the details are to be recorded on daily basis in the log book in prescribed format. Repair and maintenance of pumps shall be in the scope of contractor for the period of contract. No extra payment shall be made in this regard. Electrical connection shall be provided by BHEL at the nearest feasible location. Connection from this point till pump shall be made by contractor.  \n3.\tProviding and operating 1 number 2 HP Centrifugal pump for lifting the treated water to the raised MS tank and using the water to horticulture purposes in the nearby area in order to achieve zero liquid discharge status in BHEL Jhansi. This water is to be used for maintaining nursery at designated place and overall upkeep of the oxidation pond compound. Repair and maintenance of pumps shall be in the scope of contractor for the period of contract. No extra payment shall be made in this regard. Electrical connection shall be provided by BHEL at the nearest feasible location. Connection from this point till pump shall be made by contractor.  \nThe entire work is to be carried out as per the direction of Engineer -in- charge. The work incudes any incidental work (as per above scope), which becomes necessary for continuous operation of oxidation pond.  As the ponds are located on the peripheral area, contractor has to make proper arrangements to avoid theft of contractor’s material like pumps, electrical wires etc. \n\n",{"$f":"G7/1278000","v":1},"Per Manday",1800,710,{"$f":"F7*E7","v":1278000},{"$f":"I7/E7","v":{"$error":"#VALUE!"}},{"$f":"C7*$I$9","v":{"$error":"#VALUE!"}}]
[]
[null,"Total ",{"$f":"SUM(C7)","v":1},null,null,null,{"$f":"SUM(G7:G7)","v":1278000},null,"xx"]
[null,"Amount in words ",{"$f":"rup(I9)","v":0}]
["GST Shall be paid Extra As applicable. "]
["1. Bidder has to quote in above unlocked cell (I- 9) only. Item rate shall be calculated automatically. Calculated item rates upto four  decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
["2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT, the offer of the bidder will be rejected."]
["Penalty Clause:\n1.\tThe intent of this work is to maintain oxidation pond in running condition. Contractor has to deploy on average 50 Mandays of labour per month. If due to reasons attributable to  contractor, the labour is deployed for less than 40 Mandays for any 2 consecutive months, than penalty shall be levied @ 10% of the Monthly Bill of that 2nd Month and so on till the deployment is rectified. \n2.\tIn case of failure of any pump (Submersible or Centrifugal pump), contractor has to get the pump repaired/replaced within 15 days from the date of failure. In case of delay, penalty shall be levied @ 5% per pump on daily basis. For example if 1 pump is not working for more than 15 days, than from 16th day, daily penalty shall be levied amounting to 5% of billing of 2 Mandays. "]
[]
[null,null,"(Signature and Seal of Contractor)"]
[]
[null,null,null,null,null,"(Signature and Seal of Contractor)"]