**PR NO: M2/12/ 1200011120/BRK**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1. **JR. EXECUTIVE TABLE: QTY: 10 Nos.**   **Material Code: CG4500000712**     |  |  |  | | --- | --- | --- | |  |  |  | |  | **Jr. Executive Table**   * Steel table with Novapan or equivalent board top * Three drawers in right side and Single door at left side   With one partition inside the left drawer.   * Steel tubes are to be made out of 16 SWG material.      * Thickness steel sheets should be 18 SWG. * Steel tubes & sheets are to be painted with Olive green colour. * Provision for floor rest has to be made. * Novapan top size: 138cm x 77cm x 20mm and Table height should be 74cm. * Corner beading using PVC material. For firm grip of top, sufficient numbers of screws are to be used. |  | | |
|  | | |  | | --- | | 1. **MEDIUM BACK MAIN CHAIR – QTY: 10 Nos.**   **Material Code No. HY7802161657** | |  | |  | | **SEAT / BACK ASSEMBLY:-** The seat / back are to be made of 12 mm thick hot pressed ply wood, upholster with changeable upholstery fabric covers and moulded polyurethane foam, together with moulded back - spine cover. The back foam is to be designed with counter lumbar support for extra comfort. The Polyurethene foam is moulded with density - 45 ± 2 Kg/Cu. m and hardness = 20 ± 2 on hampden machine at 25% compression. Rear side of the Back rest and bottom of the Seat shall be covered with Black Polypropylene covers.  Seat Height : 415 mm to 530 mm  Height of Chair: 930 mm to 1050 mm  Back Rest Size: 450 mm (W) x 530 mm (H) | |  | | **ARM REST:-** Arm rest are to be made of Black integral skin polyurethane with 50 to 70 shore hardness and reinforced with MS insert. The arm rest should be scratch and weather resistant. The arm rest are to be fitted to the seat and back with arm rest connecting strip assembly, made of 0.5 Cm thick HR steel. | |  | | **PERMEANENT CONTACT MECHANISM:-** The permanent contact mechanism with 360 degree revolving facility and provision for back tilt arrangement. Required facility for tilt tension adjustment has to be provided. | |  | | **HEIGHT ADJUSTMENT:-** The Gas lift for height adjustment may be of personalized choice, with upright position locking arrangement. | |  | | **TELESCOPIC BELLOW ASSEMBLY:-** The bellow with three piece telescopic type and injuction moulded in Black poly propylene. | |  | | **PEDESTAL ASSEMBLY:-** The pedestal has to be fabricated using 0.2 Cm thick CR Steel, powder coated and fitted with an injunction moulded in Black Polypropylene hub cap. 5 Nos. of twin wheel castors are to be provided. The castor wheels made of Nylon material and twin wheel castors with hood for extra protection may be used. | |  | |