**PR NO: M2/12/ 1200011121/BRK**

1. **JR. EXECUTIVE TABLE: QTY: 3 NOS**

**Material Code: CG4500000712.**

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  | **Jr. Executive Table**   * Steel table with Novapan or equivalent board top * Three drawers in right side and Single door at left side   With one partition inside the left drawer.   * Steel tubes are to be made out of 16 SWG materials.      * Thickness steel sheets should be 18 SWG. * Steel tubes & sheets are to be painted with Olive green colour. * Provision for floor rest has to be made. * Novapan top size: 138cm x 77cm x 20mm and Table height should be 74cm. * Corner beading using PVC material. For firm grip of Novapan top, sufficient number of screws is to be used. |  |
|  |  |  |

1. **VISITOR CHAIR (NON-REVOLVING TYPE)** - **QTY: 4 NOS** **Material Code No. HY7802161665**

**SEAT / BACK ASSEMBLY:-** The seat / back are to be made of 12 mm thick hot pressed ply wood, upholster with changeable upholstery fabric covers and moulded polyurethane foam, together with moulded back - spine cover. The back foam is to be designed with counter lumbar support for extra comfort. The Polyurethane foam is moulded with density - 45 ± 2 Kg/Cu. m and hardness = 20 ± 2 on hampden machine at 25% compression. Rear side of the Back rest and bottom of the Seat shall be covered with Black Polypropylene covers.

Seat Height: 440 mm

Height of Chair: 805 mm

Width of Chair: 550 mm

Depth of Chair: 610 mm

**ARM REST:-** Arm rest are to be made of Black integral skin polyurethane with 50 to 70 shore hardness and reinforced with MS insert. The arm rest should be scratch and weather resistant. The arm rest are to be fitted to the seat and back with arm rest connecting strip assembly, made of 0.5 Cm thick HR steel.

Base of the chair shall be fixed to the frame made of black powder coated MS Pipe with suitable fixtures. Pipe outer dia shall be 25 mm. Suitable Nylon bushes shall be fixed to the bottom of the MS Pipe frame.