{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Technicalbid","Technical Bid","Price Bid"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Technicalbid","index":0,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":true,"merged":[[10,1,10,5],[1,1,1,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,5],[6,1,6,2],[6,3,6,5],[8,5,9,5]]}
[]
[null,"Bharat Heavy Electricals Limited\nPower Sector - Southern Region"]
[null,"Project - 5x800 MW Yadadri TPS"]
[null,"Volume-I Technical Bid"]
[null,"Tender No. - YTPS: SCT: 202202-72A"]
[null,{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,"Bidder's Name"]
[null,"Sl. No.","Description","UOM","Qty.","Quoted/Not Quoted"]
[null,1,"Shifting angles post from BHEL Yadadri stores, 1.5M (above GL) high fencing with angle iron post (65X65X6) placed every 2 M centre to centre embedded in rock by  drilling hole of Minimum dia 100 MM to a minimum depth of 450 MM. The drilling hole to be grouted with cement slurry mix of 1:1 after placement of angle.every 15th post last but one end post and corner post shall be strutted on both horizontal lines and 2 diagonals interoven with horizontal wire, of barbed wire of min 9.8kg per 100 RM (minimum) between the two posts fitted and fixed with GI staples , turn buckles etc. Complete rate to include cost of earth work, drilling, grouting, concrete, barbed wire and struts, labour charge etc.Complete as per standard specification, drawings, and as per instructions of BHEL Engineer incharge. painting of post (yellow color) to be included under the scope within the quoted rate.","RM",50]
[null,2,"Fencing with angle iron post placed at required distance embedded in cement concrete blocks, every 15th post and corner post shall be strutted on both sides and end posts on one side only and provided with horizontal lines and two diagonals interwoven with horizontal wires of barbed wire weghing 9.38kg per 100m (minimum), between two posts fitted and fixed with G.I. staples, turn buckles etc. complete (cost of posts, struts, earth work and concrete work to be paid for seperately). payment to be made per meter cost of total length of barbed wire used 16.18.1 with G.I. barbed wire.","RM",1500]
[null,"Note:\n(1) The above Quoted Price shall be excluding of GST, as applicable. The same shall be paid at actual .\n(2) Bidders to quote their most competitive price in Blue Colour Cell."]

{"sheet":"Technical Bid","index":1,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,4]]}
["Annexure II"]
["YTPS: SCT: 202204-95:Technical bid"]
[]
["Sl. No","Description","UOM","Qty.","Quoted/Not Quoted"]
[1,"Providing & fixing false ceiling with Thermocol thickness 50 mm at all height including providing & fixing of framework made of special section MS pipe/angles formed from pressed MS sheet and supported with GI wire grid. The cost include making of opening for light fitting grills diffusers cut out all complete as per drawings specification and direction of the Engineer in charge.","Sqm",900]
[2,"Providing Brickwork in cement mortar 1:4 (1 cement : 4 coarse sand ) in partition walls  of  115mm thickness at all height, places and position above pinth include raking out joints, curing, scaffolding etc complete excluding plastering and painting.","Sqm",135]
[3,"Providing 12 mm thick plaster in brickwork in cement mortar 1:4 on th ewall finish to the smooth Finish as per the sepcification all complete","Sqm",290]
[4,"Two coat of acrylic distemper of approved brand and manufacture to give an even even shade including a priming coal with distemper primer complete.","Sqm",85]
[]
[]
[]
[]
[null,"SIGNATURE & SEAL OF AUTHORISED PERSON"]
[]
[null,"NAME: "]

{"sheet":"Price Bid","index":2,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[[10,0,10,5],[0,0,0,5],[1,0,1,5],[2,0,2,5],[8,1,8,4],[9,2,9,5]]}
["Annexure II"]
["YTPS: SCT: 202204-95:Price bid"]
[]
["Sl. No","Description","UOM","Qty.","Unit Price (Rs.)","Total Price (Rs.)","Weigtage upto 10 Decimals"]
[1,"Providing & fixing false ceiling with Thermocol thickness 50 mm at all height including providing & fixing of framework made of special section MS pipe/angles formed from pressed MS sheet and supported with GI wire grid. The cost include making of opening for light fitting grills diffusers cut out all complete as per drawings specification and direction of the Engineer in charge.","Sqm",900,{"$f":"F5/D5","v":0},{"$f":"F9*$G$5","v":0},0.76207952757884001]
[2,"Providing Brickwork in cement mortar 1:4 (1 cement : 4 coarse sand ) in partition walls  of  115mm thickness at all height, places and position above pinth include raking out joints, curing, scaffolding etc complete excluding plastering and painting.","Sqm",135,{"$f":"F6/D6","v":0},{"$f":"F9*G6","v":0},0.14358909048692653]
[3,"Providing 12 mm thick plaster in brickwork in cement mortar 1:4 on th ewall finish to the smooth Finish as per the sepcification all complete","Sqm",290,{"$f":"F7/D7","v":0},{"$f":"F9*G7","v":0},6.7569233701397155E-2]
[4,"Two coat of acrylic distemper of approved brand and manufacture to give an even even shade including a priming coal with distemper primer complete.","Sqm",85,{"$f":"F8/D8","v":0},{"$f":"F9*G8","v":0},2.6762148232836201E-2]
[null,"Total Price (In Rs.)"]
[null,"Total Price (In Words)"]
["Note:\n(1)The above Quoted Price shall be excluding of GST, as applicable. The same shall be paid at actual .\n(2) Vendor to input their prices in blue colour cell. Total price will be calculated automatically.\n\n"]
[]
[]
[]
[null," GST - EXTRA ……….%"]
[]
[null,null,"SIGNATURE & SEAL OF AUTHORISED PERSON"]
[]
[null,null,"NAME: "]