{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["price bid "],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"price bid ","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"cut":false,"hidden":false,"merged":[[52,1,52,6],[50,1,50,6],[51,1,51,6],[48,3,48,6],[0,0,0,6],[3,0,3,6],[1,0,1,6],[2,0,2,6],[4,0,4,2],[4,4,4,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS-146)"]
["Name of work -Modification of kitchen and toilets in Type 2,3,A,B,X,H & M type of Qtrs. In Township."]
["Tender Enq No-TCX / TW / 21 / 25"]
["Sl. No.","Description of Work","% Allocation (Item-wise)","Unit ","Quantity ","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Carrige of building of rubbish",6.8648042758621755E-2,"cum",5,{"$f":"G7/E7","v":0},{"$f":"$G$48*C7%","v":0}]
[2,"Earth work in excavation by mechanical means (Hydraulic excavator)/manual means over areas (exceeding 30 cm in depth, 1.5 m in width as well as 10 sqm on plan) including getting out and disposal of excavated earth lead upto 50 m and lift upto 1.5 m, as directed by Engineer-in-charge.All kinds of soil",2.1978192642217616E-2,"cum",1,{"$f":"G8/E8","v":0},{"$f":"$G$48*C8%","v":0}]
[3,"Providing and laying in position cement concrete of specified grade excluding the cost of centering and shuttering - All work up to plinth level :  1:3:6 (1 Cement : 3 coarse sand (zone-III): 6 graded stone aggregate 40 mm nominal size). \n",2.8278055285057326,"cum",5,0,0]
[4,"Providing and laying in position cement concrete of specified grade excluding the cost of centering and shuttering - All work up to plinth level : \"1:2:4 (1 cement : 2 coarse sand (zone-III) : 4 graded stone aggregate 20 mm nominal size).",1.1292131885558789,"cum",2,0,0]
[5,"Reinforced cement concrete work in beams, suspended floors, roofs having slope up to 15° landings, balconies, shelves, chajjas, lintels, bands, plain window sills, staircases and spiral stair cases above plinth level up to floor five level, excluding the cost of centering, shuttering, finishing and reinforcement, with 1:1.5:3 (1 cement : 1.5 coarse sand (zone-III)  : 3 graded stone aggregate 20 mm nominal size).",1.6090235705864244,"cum",2,0,0]
[6,"Centering and shuttering including strutting, propping etc. and removal of form for all heights :  Suspended floors, roofs, landings, balconies and access platform .\n",0.36424993506443071,"sqm",5,0,0]
[7,"Brick work with common burnt clay F.P.S. (non modular) bricks of class designation 7.5 in superstructure above plinth level up to floor V level in all shapes and sizes in : Cement mortar 1:6 (1 cement : 6 coarse sand).\n",2.4857885551288361,"cum",3,0,0]
[8,"Half brick masonry with common burnt clay F.P.S. (non modular) bricks of class designation 7.5 in superstructure above plinth level up to floor V level. Cement mortar 1:4 (1 cement :4 coarse sand) .\n",8.3849291545742233,"sqm",85,0,0]
[9,"Providing and fixing horizontal chajja of stone 40 mm thick and upto 80 cm projection in cement mortar 1:4 (1 cement : 4 coarse sand), including pointing in white cement mortar 1:2 (1 white cement : 2 stone dust) with an admixture of pigment matching the stone shade : Red sand stone",7.5027738852305568,"sqm",50,0,0]
[10,"Providing and fixing stone slab with table rubbed, edges rounded and polished, of size 75x50 cm deep and 1.8 cm thick, fixed in urinal partitions by cutting a chase of appropriate width with chase cutter and embedding the stone in the chase with epoxy grout or with cement concrete 1:2:4 (1 cement : 2 coarse sand : 4 graded stone aggregate 6 mm nominal size) as per direction of Engineer-in-charge and finished smooth. White Agaria Marble Stone. \n",2.3724494848386675,"sqm",5,0,0]
[11,"Cement concrete flooring 1:2:4 (1 cement : 2 coarse sand : 4 graded stone aggregate) finished with a floating coat of neat cement, including cement slurry, but excluding the cost of nosing of steps etc. complete.  40 mm thick with 20 mm nominal size stone aggregate. \n",4.2665090123241024E-2,"sqm",1,0,0]
[12,"Providing and fixing Ist quality ceramic glazed wall tiles conforming to IS: 15622 (thickness to be specified by the manufacturer), of approved make, in all colours, shades except burgundy, bottle green, black of any size as approved by Engineer-in-Charge, in skirting, risers of steps and dados, over 12 mm thick bed of cement mortar 1:3 (1 cement : 3 coarse sand) and jointing with grey cement slurry @ 3.3kg per sqm, including pointing in white cement mixed with pigment of matching shade complete. ",27.725764854627641,"sqm",250,0,0]
[13,"Providing and laying Ceramic glazed floor tiles of size 300x300 mm (thickness to be specified by the manufacturer), of 1st quality conforming to IS : 15622, of approved make, in all colours, shades, except White, Ivory, Grey, Fume Red Brown, laid on 20 mm thick bed of cement mortar 1:4 (1 Cement : 4 Coarse sand), jointing with grey cement slurry @ 3.3kg/sqm  including pointing the joints with white cement and matching pigments etc., complete. ",17.184416405695618,"sqm",160,0,0]
[14,"Providing and fixing on wall face unplasticised Rigid PVC rain water pipes conforming to IS : 13592 Type A, including jointing with seal ring conforming to IS : 5382, leaving 10 mm gap for thermal expansion, (i) Single socketed pipes.  75 mm diameter ",0.85246420560350533,"m",36,0,0]
[15,"Providing and fixing on wall face unplasticised Rigid PVC rain water pipes conforming to IS : 13592 Type A, including jointing with seal ring conforming to IS : 5382, leaving 10 mm gap for thermal expansion, (i) Single socketed pipes.  110 mm diameter. ",1.5531558599367035,"m",42,0,0]
[16,"15 mm (1:6) Plaster",2.3065934316177623,"sqm",85,0,0]
[17,"Providing and applying plaster of paris putty of 2 mm thickness over plastered surface to prepare the surface even and smooth complete.",2.4516460130694768,"sqm",120,0,0]
[18,"Distempering with oil bound washable distemper of approved brand and manufacture to give an even shade :  New work (two or more coats) over and including water thinnable priming coat with cement primer.\n",1.9178874131963903,"sqm",120,0,0]
[19,"Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc. complete. ",0.16046959868029628,"sqm",110,0,0]
[20,"Painting with synthetic enamel paint of approved brand and manufacture of required colour to give an even shade :One or more coats on old work",0.42891939273180546,"sqm",50,0,0]
[21,"Dismantling G.I. pipes (external work) including excavation and refilling trenches after taking out the pipes, manually/ by mechanical means including stacking of pipes within 50 metres lead as per direction of Engineer-in-charge : 15 mm to 40 mm nominal bore.\n",0.77748183658118764,"m",70,0,0]
[22,"Dismantling old plaster or skirting raking out joints and cleaning the surface for plaster including disposal of rubbish to the dumping ground within 50 metres lead. ",0.8403888508528784,"sqm",215,0,0]
[23,"Demolishing brick work manually/ by mechanical means including stacking of serviceable material and disposal of unserviceable material within 50 metres lead as per direction of Engineer-in-charge.In cement mortar",2.2058898589792255,"sqm",15,0,0]
[24,"Demolishing R.C.C. work manually/ by mechanical means including stacking of steel bars and disposal of unserviceable material within 50 metres lead as per direction of Engineer - in- charge.",0.25381802388040992,"cum",1,0,0]
[25,"Demolishing cement concrete manually/ by mechanical means\nincluding disposal of material within 50 metres lead as per direction of Engineer - in - charge. Nominal concrete 1:3:6 or richer mix (i/c equivalent design mix)",0.17398457303630865,"cum",1,0,0]
[26,"Taking out doors, windows and clerestory window shutters (steel or wood) including stacking within 50 metres lead : Of area 3 sq. metres and below",3.2064254847221016E-2,"each",3,0,0]
[27,"Dismantling of flushing cistern of all types (C.I./PVC/Vitrious China) including stacking of useful materials near the site and disposal of unserviceable materials within 50 metres lead.",0.47784900938029945,"Nos",7,0,0]
[28,"Providing and fixing water closet squatting pan (Indian type W.C. pan ) with 100 mm sand cast Iron P or S trap, 10 litre low level white P.V.C. flushing cistern, including flush pipe, with manually controlled device (handle lever) conforming to IS : 7231, with all fittings and fixtures complete, including cutting and making good the walls and floors wherever required: White Vitreous china Orissa pattern W.C. pan of size 580x440 mm with integral type foot rests. \n",4.4561828215689205,"nos",8,0,0]
[29,"Providing and fixing white vitreous china pedestal type water closet (European type) with seat and lid, 10 litre low level white vitreous china flushing cistern & C.P. flush bend with fittings & C.I. brackets, 40 mm flush bend, overflow arrangement with specials of standard make and mosquito proof coupling of approved municipal design complete, including painting of fittings and brackets, cutting and making good the walls and floors wherever required : W.C. pan with ISI marked white solid plastic seat and lid.\n",0.72821194620778429,"nos",1,0,0]
[30,"Providing and fixing wash basin with C.I. brackets, 15 mm C.P. brass pillar taps, 32 mm C.P. brass waste of standard pattern, including painting of fittings and brackets, cutting and making good the walls wherever require:  White Vitreous China Wash basin size 630x450 mm with a single 15 mm C.P. brass pillar tap.\n",1.5950287230286169,"nos",5,0,0]
[31,"Providing and fixing white vitreous china pedestal for wash basin completely recessed at the back for the reception of pipes and fittings. ",0.74206719428870604,"nos",5,0,0]
[32,"Providing and fixing P.V.C. waste pipe for sink or wash basin including P.V.C. waste fittings complete. Semi rigid pipe  40 MM dia.\n",6.557685426713282E-2,"each",5,0,0]
[33,"Providing and fixing 100 mm sand cast Iron grating for gully trap. ",4.0728147381449711E-2,"nos",10,0,0]
[34,"Providing and fixing 600x450 mm beveled edge mirror of superior glass (of approved quality) complete with 6 mm thick hard board ground fixed to wooden cleats with C.P. brass screws and washers complete.",0.65445979757552331,"each",5,0,0]
[35,"Providing and fixing wash basin with C.I. brackets, 15 mm C.P. brass pillar taps, 32 mm C.P. brass waste of standard pattern, including painting of fittings and brackets, cutting and making good the walls wherever require:White Vitreous China Flat back wash basin size 450x 300 mm with single 15 mm C.P. brass pillar tap",0.75112022036475401,"each",3,0,0]
[36,"Providing and fixing G.I. pipes complete with G.I. fittings and clamps, i/c cutting and making good the walls etc.  15 mm dia nominal bore.\n",1.4884794222954845,"m",50,0,0]
[37,"Providing and fixing brass stop cock of approved quality: 15 mm nominal bore.",0.19430502189050666,"nos",5,0,0]
[38,"Providing and fixing C.P. brass bib cock of approved quality conforming to IS:8931 :  15 mm nominal bore.\n",0.55534416898656258,"nos",10,0,0]
[39,"Providing and fixing C.P. brass long body bib cock of approved quality conforming to IS standards and weighing not less than 690 gms.  15 mm nominal bore.\n",0.36753924773855379,"nos",5,0,0]
[40,"Providing and fixing C.P. brass stop cock (concealed) of standard design and of approved make conforming to IS:8931. 15 mm nominal bore. \n",0.81264345482181366,"nos",10,0,0]
[41,"Items cover in DSR-2016 but not covered above ",1.3959947688586021,"Dsr-2016",8000,0,0]
[null,"Total ",{"$f":"SUM(C7:C47)","v":99.999999999999943}]
[null,"IN WORDS",null,{"$f":"rup(G48)","v":0}]
[null,"Note -GST extra as applicable"]
[null,"1. Bidder has to quote in above unlocked cell (G48) only and take print out  to submitt alongwith Tech-bid. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"3.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[]
[null,null,null,"(Signature and Seal of  Contractor  )"]