{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["price bid "],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"price bid ","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[[19,1,19,6],[17,1,17,6],[18,1,18,6],[15,3,15,6],[0,0,0,6],[3,0,3,6],[1,0,1,6],[2,0,2,6],[4,0,4,2],[4,4,4,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID"]
["Name of work -Misc.Civil and Modification works  in guest house ."]
["Tender Enq No-TCX / TW / 21 / 21"]
["Sl. No.","Description of Work","% Allocation (Item-wise)","Unit ","Quantity ","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Providing and applying plaster of paris putty of 2 mm to 5 mm thickness over plastered surface to prepare the surface even and smooth complete.",3.5929511323385639,"sqm",147,{"$f":"G7/E7","v":0},{"$f":"ROUND($G$15*C7%,2)","v":0}]
[2,"Providing and fixing aluminium work  heavy duty for doors, windows, ventilators and partitions with extruded built up standard tubular sections/ appropriate Z sections and other sections of approved make conforming to IS: 733 and IS: 1285, fixing with dash fasteners of required dia and size, including necessary filling up the gaps at junctions, i.e. at top, bottom and sides with required EPDM rubber/ neoprene gasket etc. Aluminium sections shall be smooth, rust free, straight, mitred and jointed mechanically wherever required including cleat angle, Aluminium snap beading for glazing / paneling, C.P. brass / stainless steel screws, all complete as per architectural drawings and the directions of Engineer-in-charge.",18.153078069655251,"kg",221,{"$f":"G8/E8","v":0},{"$f":"ROUND($G$15*C8%,2)","v":0}]
[3,"P/Fixing extra large (size as per approved) premium tiles make-Kajaria in all colour and shade in wall / skirting / riser of steps laid with cement based high polymer modified quick set tile adhesive (water based ) conforming to IS : 15477, in average 6mm thickness, including grouting of joints complete all as specified and as directed by engineer -in-charge(The measurement shall be taken actual at site, any wastage should be included in the rate quoted.)",10.247543794977002,"sqm",31,{"$f":"G9/E9","v":0},{"$f":"ROUND($G$15*C9%,2)","v":0}]
[4,"P/F 12 mm thick toughned glass door shutters including necessary joining cleats, glazing clips, stainless steel handle and suitable lock for toughened glass, necessary pivot stainless steel, floor spring(Double spindle) capacity upto 120 kg foundation box for each shutter, necessary frame work and all fittings etc. complete all as specified and as directed by engineer -in-charge(The measurement shall be taken actual at site, any wastage should be included in the rate quoted.)",12.32109371243569,"sqm",15,{"$f":"G10/E10","v":0},{"$f":"ROUND($G$15*C10%,2)","v":0}]
[5,"P/F 12 mm thick toughned glass fixed with steel connectors, top and bottom pivots including including as partition wall, including all necessary fittings all as directed by engineer-in-charge as specified.(The measurement shall be taken actual at site, any wastage should be included in the rate quoted.)",32.034843652332796,"sqm",41,{"$f":"G11/E11","v":0},{"$f":"ROUND($G$15*C11%,2)","v":0}]
[6,"False ceiling / moulding /boarder top desing including POP punning of existent ceiling of design as per approved by engineer-in-charge.",18.842257945602874,"rm",57,{"$f":"G12/E12","v":0},{"$f":"ROUND($G$15*C12%,2)","v":0}]
[7,"Providing and applying plaster of paris putty of 15 mm to 20 mm thickness over plastered surface to prepare the surface even and smooth complete  as per direction of engineer-in-incharge.",1.4424695077973493,"sqm",16,{"$f":"G13/E13","v":0},{"$f":"ROUND($G$15*C13%,2)","v":0}]
[8,"P/F Suspended PVC false ceiling including all fittings/hardware etc. of grid for fixing….design and colour as per approved by engineer-in-charge",3.3657621848604813,"sqm",14,{"$f":"G14/E14","v":0},{"$f":"ROUND($G$15*C14%,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C14)","v":100.00000000000003}]
[null,"IN WORDS",null,{"$f":"rup(G15)","v":0}]
[null,"Note -GST extra as applicable"]
[null,"1. Bidder has to quote in above unlocked cell (I15) only and take print out  to submitt alongwith Tech-bid. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"3.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[]
[null,null,null,"(Signature and Seal of  Contractor  )"]