Bharat Heavy Electricals Limited

(A Govt. Of India Undertaking)
POWER SECTOR, PROJECT ENGINEERING MANAGEMENT

Power Project Engg. Institute, Plot No. 25, Sector 16 - A,

HRDI & ESI Complex, NOIDA 201 301 (UP)

                 PROJECT INFORMATION
4 X 270 MW BHADRADRI TPS 
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These Conditions shall be read in conjunction with General Condition of Contract (GCC) and Corrigendum to GCC rev-06 enclosed along with the tender enquiry. In case of any conflict or inconsistency, the requirement of project information shall prevail over the GCC and Corrigendum to GCC rev-06.

	1.0
	Project Name
	4X270 MW TSGENCO BHADRADRI TPS

	2.0
	Ultimate Customer 
	TSGENCO

	3.0
	Location  of Plant
	The distance from Manuguru to Major cities in state: Hyderabad-345KM, Warangal-180km, Bhadrachalam-38km, Kothagudem-70km and Khammam-130km, Vijayawada-195km.

Village: RAMANUJAVARAM
District: KHAMMAM
State : TELANGANA,
Nearest Airport: The nearest airport is Vijayawada Airport but the most used airport is the Hyderabad International Airport.
Nearest Railway Station: Manuguru railway station is 10KM from nearby town.  However Warangal/Vijayawada railway Station is major railway station near to Manuguru.

	4.0
	Consignee Address / BHEL Site Office Address
	Construction Manager,
Bharat Heavy Electrical Limited site office,

BTPS Manuguru,

Khammam District,

Telangana - 507117

	
	   Notes:
	1. Consignee address in LR should be strictly as per Sl. No. 04.
2. Vendor to note that to effect “Sale in Transit”, BHEL shall issue “Delivery Order” to the Transporter for transferring the ownership from BHEL to customer (TSGENCO).

3. It is Vendor's responsibility to ensure availability of trucks well in advance for dispatch of material to meet contractual delivery requirement.

Delivery Order  shall be carried by transporter along with other dispatch documents.

	5.0
	Mode of Dispatch
	By Road/Rail/Sea on Door Delivery and freight Pre-Paid Basis. 

	6.0
	Transit Insurance
	In BHEL Scope.

Vendor shall inform the following details of dispatches to the Underwriter (refer details below) under intimation to BHEL-PEM and BHEL Site office: 
(1) Policy No. 

(2) Consignee Name.
(3) Consignment Details (items with their weights and value (in INR)).
(4) Project Name and P.O. No. 
(5) LR No. and date, Despatch origin and destination details, Inv. No.

	
	Policy No.   
	  500300/21/15/02/00000031 (Marine policy)

  500300/44/15/04/40000014 (SCE Policy no)  

	
	Name of the insurance company details:                                                                              
	Mr. Ashim Mukherjee (CRM)

United India Insurance Co. Ltd (UIIC)

(A company wholly owned by Govt. of India)
D-24 & E-25, 2nd Floor, 

Himalaya House, 23, KG Marg,

New Delhi, Pin - 110001.

Mb. No. 09899720652, Telephone no.: 01123318077, 41521760
E-mail id: (akmukherjee@uiic.co.in, corpcelldel@uiic.co.in)

	7.0
	Unloading at site
	· By BHEL site office for Supply packages. (The Vendor shall furnish LR wise Gross Wt. and net weight of the consignment in attached format annex-II for the purpose of handling the consignment by BHEL site loading/unloading contractor).
· By Vendor for Turnkey i.e. Supply and Erection & Commissioning Packages.

	8.0
	Storage at site
	· By BHEL site for Supply packages.

· By Vendor for Turnkey i.e. Supply and Erection & Commissioning Packages.

	9.0
	Movement of Material within Site
	· By BHEL site for Supply packages.
· By Vendor for Turnkey i.e. Supply and Erection & Commissioning Packages.

	10.0
	Provision of facilities at Site (Applicable for Turnkey Packages)


	Construction Power: it will be provided at one point of plant boundary free of cost.
Construction Water: it will be provided at one point of plant boundary free of cost.

	11.0
	Inspection Agency 
(Domestic & Imported supply supplies)
	Later

	12.0
	Packing, Identification & marking
	· The supplier shall include and provide for securely protecting and packing the materials so as to avoid loss or damage during handling & transport by air, sea, rail and road.

·  All packing shall allow for easy removal and checking at site. Special precaution shall be taken to prevent rusting of steel and iron parts during transit by sea. Gas seals or other materials shall be adopted by the Contractor for protection against moisture during transit.

· The number of each package in a shipment shall be shown in fraction, numerator showing number of the package and the denominator showing total number of packages in a lot / consignment. The packages number shall be generally prepared in the sequence in which they will be required for erection.

	
	
	· Each package delivered under the Contract shall be marked by and at the expense of the supplier and such marking must be distinct and in English language (all previous irrelevant markings being carefully obliterated). Such marking shall show the description and quantity of contents, the name and address of consignee, the gross weight and net weight of the package, the name of the Contractor with a distinctive number of mark sufficient for purposes of identification. All markings shall be carried out with such materials as to ensure quickness of drying, fastness and indelibility. Each equipment or parts of equipment shall, when shipped or railed or otherwise dispatched be tagged with reference to the assembly drawings and corresponding part numbers. Each bale or package shall contain a packing note quoting specifically the name of the Contractor, the number and date of contract and the name of the office placing the contract, nomenclature of the stores and include a schedule of parts for each complete equipment giving the part numbers with reference to the assembly drawing and the quantity of each part, drawings nos. and tag numbers.

· Rotor bearings should not be used as a support while packing.

· Besides wherever necessary, packing shall bear a special marking "TOP","BOTTOM", "DO NOT TURN OVER", "KEEP DRY", "HANDLE WITH CARE",etc.

· All packing cases, containers (excluding marine container), packing and other similar materials shall be new.

· Notwithstanding anything stated in this clause, the Contractor shall be entirely responsible for loss, damage or depreciation or deterioration to the materials & supplies due to faulty and/or insecure packing.

· One copy of respective standard manufacturer's erection instruction/operation instruction manual shall be kept in each package/container for immediate reference.

	
	
	· Each and every package box shall be marked with the following, as a minimum:

(i). Name and address of Consignee :

(ii). Project reference :

(iii). Contract No.:

(iv). Packing No.: (1/10, 2/10, 3/10 ...... when there are 10 packages 

For one consignment)

(v). Net Weight/Gross Weight :

(vi). Port of Loading :

(vii). Destination Port : Chennai

(viii). Packing Mark : [symbols indicating "TOP" and other special  

markings as per clause 10.10.(4) & 10.10.(6) above]

(ix). Type of Equipment :

       "E" (for Equipment supply)

       "T" (for Tools & Tackles)

       "S" (for Mandatory Spares)

· Two copies of packing list should be kept in case/package No. 1 of each consignment of the goods and four copies in each case (three inside the box and one copy in a special packet at the outer side of the Box).

	13.0
	Commissioning spares
	The commissioning spares shall be properly packed separately in separate box and each spare shall be properly tagged giving details (to match the description given in the packing slip) to facilitate their proper identification. Three copies of packing list is to be kept inside the box and one copy in a special packet at the outer side of the Box.

	14.0
	Mandatory Spares


	The Mandatory spares shall be properly packed separately in separate box indicating Mandatory Spares in bold letters and each spare shall be properly tagged giving details i.e. item number of the equipment in line with the Ultimate Customer Contract & Number per item (to match the description given in the packing slip) to facilitate their proper identification by ultimate customer M/s TSGENCO. Three copies of packing list along with Manufacturing drawing no. Reference, Catalogue reference etc. is to be kept inside the box and one copy in a special packet at the outer side of the Box.

	15.0


	Submission of Final Drawing / Documents along with O&M Manual, Type Test Certificates (if any) 
	As per GCC/ Technical specification/ Kickoff meeting.
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