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Serrated Gasket

 (For internal reference only)

Remove this preface sheet before issuing to supplier.

         Designation:  Serrated Gasket


Material specification column           :   TC 51347


Description column     
  :  Serrated Gasket 


Material code column
  :  As per Variant Table


ON INDENTS :


Material specification column
 :
 TC 51347


Description column
 :
 A Serrated Gasket of nominal diameter 200 mm and    nominal pressure rating160 shall be designated as Serrated Gasket  DN 200  PN160.   


Material code column
 :
 As given in the Variant Table


ON ENQUIRES & PURCHASE ORDERS : 


A copy of this standard shall be enclosed without the preface sheet.

SERRATED GASKET

1.0  SCOPE:



This standard applies to serrated gaskets used to seal the flange connections of steam turbines.

2.0 TECHNICAL SPECFICATION:

1) Description          : Serrated Gasket

2) Profile                  : B 25 A/ Kempchen Werknorm 145

3) Nominal Size       : Refer variant table

4) Nominal Pressure: Refer variant table

5) Material               : 1.4541/Graphite face ( Auflage Graphit)

6) Gasket thickness  : 4 mm+2x0.5 mm graphite

3.0) DIMENSIONS: As specified in the variant table.

4.0) TEST AND GUARANTEE  CERTIFICATES :

4.1
    TEST CERTIFICATES :  

Three copies of test certificates are to be given for each consignment. BHEL Standard number and purchase order no. shall be mentioned in the test certificates.


4.2
GUARANTEE CERTIFICATE :   A guarantee certificate for 24 months of 



trouble free performance from the date of shipment or 12 months from the date of commissioning whichever is earlier shall be supplied.

5.0
DOCUMENTS :   Technical literature shall accompany the offer.


6.0
PACKING : The material shall be properly packed to ensure that it is capable of with



standing transit risks without damage.
7.0  MARKING : 
A tag bearing relevant 12 digit material code of BHEL and Purchase Order number shall be attached to the supply. Product name and manufacturer’s name has to be clearly indicated on the product.


Following details shall be marked on the packing case.

a) Manufacturer’s name.

:

b) BHEL order number.

:

c) BHEL standard number

:    

8.0 VARIANT TABLE :




For DIN flanges



	VARIANT
	DESCRIPTION


	d1

(mm)
	d2

(mm)
	d3

(mm)
	MATERIAL CODE

	01
	Serrated Gasket 
	DN 200 PN160
	220
	248
	324
	TC9751347017

	02
	Serrated Gasket
	DN 150 PN64
	174
	200
	247
	TC9751347025

	03
	Serrated Gasket
	DN 100 PN64
	120
	144
	174
	TC9751347033

	04
	Serrated Gasket
	DN 150 PN40
	174
	196
	224
	TC9751347041

	05
	
	
	
	
	
	

	06
	
	
	
	
	
	

	07
	
	
	
	
	
	

	08
	
	
	
	
	
	


RECORD OF REVISIONS

	REV. NO.
	DATE
	REVISION DETAILS
	REVISED
	APPROVED

	00


	23-09-2003
	NEW SPEC.
	MRB
	A.GUPTA



	01


	13-01-2004
	Variant 02,03&04 added
	RRKR
	S.M.K
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