ANNEXURE: I

SCOPE OF WORK OF REPAIRNG & SERVICING OF CEE DEE VACUUM PLANT (CT PROCESSING PLANT) WITH SUPPLY OF 2 NO FAN BLOWER ASSEMBLY IN BAY-6 TRM BL.III.

1. Dismantle of centrifugal blower (Dully Assembled).

2. Repair/replacement of motor/motor bearings.

3. Repair/replacement of blower bearings.

4. Repair/replacement of pedestal block.

5. Assemble of centrifugal blower (Dully Assembled).

5. Check the proper movement and balancing of blower.

6. Repair/replacement of drive brakes.

7. Repair/replacement of all nut & bolts.

8. Repair/replacement of all other damaged parts like shaft & bearings (CENTRIFUGAL BLOWER SHAFT 2 NO (Material EN 8)).

9. Repair/replacement of pully.

10. Checking the greasing and oiling of process plant.

11. All material will be providing by BHEL BHOPAL EXPECT 2 NOS ENTRIFUGAL BLOWER (50000 CUB M/HR, STATIC PRESSURE 60 MM @ 150 deg C, ANTTICLOCK WISE WITH 25 HP, RPM 1440(DULLY ASSEMBLED).

12. The time period the completing the work shall be Four Month from the date of issue of work order.

**Scope of Supply of Contractor:**

* CENTRIFUGAL BLOWER 2 NO (50000 CUB M/HR, STATIC PRESSURE 60 MM @ 150 degC, ANTTICLOCK WISE WITH 25 HP, RPM 1440(DULLY ASSEMBLED**.**

Ram Pratap Seth

Dy .Mgr(FRX**)**