**BHARAT HEAVY ELECTRICALS LTD, BHOPAL**

**MATERIAL MANAGEMENT (SCR)**

**PIPLANI – BHOPAL - 462022 (M.P.)**

**PHONE NO: +91 755 2503637/+91 755 2505087**

**Email:** sahirwar@bhel.in **/** atulchaturvedi@bhel.in

**TENDERS ARE INVITED FOR SUPPLY OF FOLLOWING ITEM FROM VENDORS:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SL****NO** | **ENQ. NO.** | **IT. NO.** | **ITEM DESCRIPTION** | **QTY** | **TENDER FEE** | **DUE DATE** |
| **1** | **E4843087** | **1** | HAND THROTTLE ASSY COMPLETE WITH DUAL GANG POTS EACH OF 1 K OHM, 25W RATING (OHMITE). THE ASSY TO BE COMPLETE WITH HANDWHEEL, BRASS BLOCK, HAND THROTTLE KIT WITH STOP PIN AND 2 NOS AUXILIARY SWITCH DT-2RV3-B6 OF HONEYWELL. ASSEMBLY SHALL BE AS PER HILLGRAHAM PART NOS. Z923+Z922+Z928+R995+S302+S302) OR NOV (ROSSHILL) PART NOS 0001-0007-09 + 2 NOS OF 1704-1603-01 OR EQUIVALENT.HAND THROTTLE WHEEL TO BE OF SOLID STAINLESS STEEL | **10 NO.** | **Not Applicable** | **04/01/25** |
| **2** | **E4843087** | **2** | RESISTER 1K, 25W, DUAL GANG IMPORTED FOR HAND THROTTLE TO HILL GRAHAM PART NO: R995 OR EQUIVALENT. | **15 NO.** | **Not Applicable** | **04/01/25** |
| **3** | **E4843087** | **3** | SWITCH HAND THROTTLE MICRO SWITCH(HTMS), 2 C/O TYPE DT2RV AS PER HGC PART NO S302 OR EQUIVALENT. | **15 NO.** | **Not Applicable** | **04/01/25** |
| **4** | **E4843087** | **4** | OIL RIG SCR PANEL TWIN (DUPLEX) BLOWER WITH 600V AC 50 HZ MOTOR AS PER BHEL SPECIFICATION NO. OR 12032, REV. 01 (AS PER HILL GRAHAM PART NO. B103 OR EQUIVALENT) | **15 NO.** | **Not Applicable** | **04/01/25** |
| **5** | **E4843087** | **5** | FOOT THROTTLE ASSEMBLY COMPLETE WITH PEDAL SWITCH, 200 OHM HALF MOON POTENTIOMETER AS PER BHEL SPECIFICATION NO-OR12063 REV 02 & OR 12135 REV 00. THE FOOT THROTTLE ASSEMBLY SHALL BE EXACT EQUIVALENT TO HILL GRAHAM PART NO-F098 OR MODEL 201 OF NOV (ROSSHILL) USA. | **05 NO.** | **Not Applicable** | **04/01/25** |
| **6** | **E4843087** | **6** | EDGE WISE ANALOG METER SCALE 0-100% , BASIC 0-1 MA EQUIVALENT TO HGC(ZEEFAX) PART NO.M150 ,SUITABLE FOR 31X65 MM CUTOUT (FOR POWER LIMIT DISPLAY IN DRILLERS CONSOLE) | **10 NO.** | **Not Applicable** | **04/01/25** |

1. Complete tender document and details can be downloaded from [**https://eprocurebhel.co.in**](https://eprocurebhel.co.in/)
2. Bids are invited in two parts through EPS ([**https://eprocurebhel.co.in**](https://eprocurebhel.co.in/)). Part-1 will consist Pre-Qualification criteria, technical specifications of the item and commercial terms & conditions, Part-2 will be the Price bids. The bids to be submitted not later than **01:00 PM** (IST) on the due date. Tenders will be opened on due date from **05:00 PM** (IST) onwards.
3. All subsequent corrigendum/amendment shall be published only on the e-procurement website. Hence, bidders are advised to be in touch with the e-procurement website till the tender is finally opened.
4. Price bids of techno-commercially qualified vendors will only be opened which will be suitably notified.
5. BHEL reserves the right to accept or reject any of the bid / all the bids or cancel or withdraw the invitation of tender without assigning any reason whatsoever and in such case no bidder / intending bidder shall have any claim arising out of such action by BHEL.
6. BHEL’s “GENERAL TERMS AND CONDITIONS OF ENQUIRY” BP200102B, available on vendor’s portal at [**https://bpl.bhel.com/bplweb\_new**](https://bpl.bhel.com/bplweb_new) shall prevail.