{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[[14,3,14,5],[15,2,15,6],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[17,0,20,0],[17,1,17,6],[18,1,18,6],[19,1,19,6],[20,1,20,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:  Increasing the height of existing boundary wall on the southern periphery of the Township Premises of BHEL TP Jhansi"]
["Tender Enq No-TCX/TW/22/16"]
["Sl. No.","Description of Work","Itemwise % Allocation","Unit ","Quantity ","Rate (Rs.)","Amount (Rs.)"]
[1,"Earth work in excavation by mechanical means (Hydraulic excavator) / manual means over areas (exceeding 30cm in depth. 1.5 m in width as well as 10 sqm on plan) including disposal of excavated earth, lead upto 50m and lift upto 1.5m, disposed earth to be levelled and neatly dressed (All kinds of soil)",2.0884470999999998E-3,"Cum",10,{"$f":"+ROUND(G7/E7,2)","v":0},{"$f":"+ROUND(C7*G15,2)","v":0}]
[2,"Providing and laying in position cement concrete of specified grade excluding the cost of centering and shuttering - All work up to plinth level : 1:3:6 (1 Cement : 3 coarse sand (zone-III): 6 graded stone aggregate 40 mm nominal size).",5.3738969999999999E-3,"Cum",1,{"$f":"+ROUND(G8/E8,2)","v":0},{"$f":"+ROUND(C8*G15,2)","v":0}]
[3,"Providing and laying in position specified grade of reinforced cement concrete, excluding the cost of centering, shuttering, finishing and reinforcement - All work up to plinth level :  1:2:4 (1 cement : 2 coarse sand : 4 graded stone aggregate 20 mm nominal size) ",5.8467644999999997E-3,"Cum",1,0,{"$f":"+ROUND(C9*G15,2)","v":0}]
[4,"Random rubble masonry with hard stone in superstructure above plinth level and upto floor five level, including leveling up with cement concrete 1:6:12 (1 cement: 6 coarse sand : 12 graded stone aggregate 20 mm nominal size) at window sills,ceiling level and the like. Cement mortar 1:6 (1 cement : 6 coarse sand.",0.72160543129999999,"Cum",107,0,{"$f":"+ROUND(C10*G15,2)","v":0}]
[5,"Pointing on stone work with cement mortar 1:3 (1 cement : 3 fine Raised and cut pointing",0.23133757520000001,"Sqm",477,0,{"$f":"+ROUND(C11*G15,2)","v":0}]
[6,"Demolishing stone rubble masonry manually/ by mechanical means including stacking of serviceable material and disposal of unserviceable material within 50 metres lead as per direction of Engineer-in-charge :cement mortar",1.3340108099999999E-2,"Cum",8,0,{"$f":"+ROUND(C12*G15,2)","v":0}]
[7,"Removing mortar from and cleaning stones and concrete articles(net quantity of stacks of cleaned materials will be measured):In cement mortar",3.7711831E-3,"cum",8,0,{"$f":"+ROUND(C13*G15,2)","v":0}]
[8," Not covered in above but covered in  DSR-2016",1.6636593700000001E-2,"LS",10000,0,{"$f":"+ROUND(C14*G15,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C14)","v":1},"Total amount quoted by bidder"]
[null,"IN WORDS",{"$f":"rup(G15)","v":0}]
[]
["Note:","1. GST extra as applicable"]
[null,"2. Bidder has to quote in above unlocked cell (G-15) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"3. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"4. The quantity of items in the BOQ are only tentative and approximate and are liable for variation up to any extent provided the total value of the Contract does not vary by more than 30% (Thirty percent)."]
[]
[null,null,null,"(Signature and Seal of Contractor)"]