{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price Bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price Bid","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[[21,3,21,5],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[22,2,22,6],[24,0,27,0],[24,1,24,6],[25,1,25,6],[26,1,26,6],[27,1,27,6]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["TOWNSHIP CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:  Miscellaneous Repair and Maintenance works of Boundary wall in the Township Premises of BHEL TP Jhansi"]
["Tender Enq No-TCX/TW/24/10"]
["Sl.no.","Descripition of work","% Allocation (Item-wise) ","Unit","Qty.","Rate (Rs.)","Amount (Rs.)"]
[1,"Earth  work  in  excavation  by mechanical  means  (Hydraulic excavator)  /  manual  means  in  foundation  trenches or drains, All kinds of soil  (not exceeding 1.5 m in width or 10 sqm on plan) including dressing of sides and ramming of bottoms, lift upto 1.5 m, including getting out the  excavated  soil  and  disposal  of  surplus excavated  soil  as directed, within a lead of 50 m. ",1.3408261600000001E-2,"Cum",44,{"$f":"+ROUND(G7/E7,2)","v":0},{"$f":"+ROUND(C7*G22,2)","v":0}]
[2,"Providing and laying in position cement concrete of specified grade excluding the cost of centering and shuttering - All work up to plinth level : 1:4:8 (1 Cement : 4 coarse sand (zone-III) : 8 graded stone\naggregate 40 mm nominal size)",2.3739698E-2,"Cum",4,0,{"$f":"+ROUND(C8*G22,2)","v":0}]
[3,"Providing and laying in position specified grade of reinforced cement concrete, excluding the cost of centering, shuttering, finishing and reinforcement - All work up to plinth level :  1:2:4 (1 cement : 2 coarse sand : 4 graded stone aggregate 20 mm nominal size) ",3.9075066899999997E-2,"Cum",6,0,{"$f":"+ROUND(C9*G22,2)","v":0}]
[4,"Providing and laying in position specified grade of reinforced cement concrete, excluding the cost of centering, shuttering, finishing and reinforcement - All work up to plinth level :1:1.5:3 (1 cement : 1.5 coarse sand (zone-III): 3 graded stone\naggregate 20 mm nominal size).",2.5375397899999999E-2,"Cum",4,0,{"$f":"+ROUND(C10*G22,2)","v":0}]
[5,"Centering and shuttering including strutting, propping etc. and removal of form for all heights :Foundations, footings, bases of columns, etc. for mass concrete.  ",6.4167013E-3,"sqm",19,0,{"$f":"+ROUND(C11*G22,2)","v":0}]
[6,"Centering and shuttering including strutting, propping etc. and removal of form for all heights : Lintels, beams, plinth beams, girders, bressumers and cantilevers",6.1017679999999998E-4,"sqm",1,0,{"$f":"+ROUND(C12*G22,2)","v":0}]
[7,"Steel reinforcement for R.C.C. work including straightening, cutting, bending, placing in position and binding all complete upto plinth level. Thermo-Mechanically Treated bars of grade Fe-500D or more.",7.7054287599999993E-2,"kg",848,0,{"$f":"+ROUND(C13*G22,2)","v":0}]
[8,"Random rubble masonry with hard stone in foundation and plinth including levelling up with cement concrete 1:6:12 (1 cement : 6 coarse sand : 12 graded stone aggregate 20 mm nominal size) upto plinth level with : Cement mortar 1:6 (1 cement : 6 coarse sand) ",0.2076243314,"Cum",34,0,{"$f":"+ROUND(C14*G22,2)","v":0}]
[9,"Random rubble masonry with hard stone in superstructure above plinth level and upto floor five level, including leveling up with cement concrete 1:6:12 (1 cement: 6 coarse sand : 12 graded stone aggregate 20 mm nominal size) at window sills,ceiling level and the like. Cement mortar 1:6 (1 cement : 6 coarse sand.",0.35305768459999998,"Cum",47,0,{"$f":"+ROUND(C15*G22,2)","v":0}]
[10,"20 mm cement plaster of mix : 1:6 (1 cement: 6 fine sand)   ",8.5799236000000001E-2,"sqm",240,0,{"$f":"+ROUND(C16*G22,2)","v":0}]
[11,"Pointing on stone work with cement mortar 1:3 (1 cement : 3 fine Raised and cut pointing",2.7551377799999999E-2,"Sqm",51,0,{"$f":"+ROUND(C17*G22,2)","v":0}]
[12,"Demolishing stone rubble masonry manually/ by mechanical means including stacking of serviceable material and disposal of unserviceable material within 50 metres lead as per direction of Engineer-in-charge :cement mortar",1.4859274800000001E-2,"Cum",8,0,{"$f":"+ROUND(C18*G22,2)","v":0}]
[13,"Removing mortar from and cleaning stones and concrete articles(net quantity of stacks of cleaned materials will be measured):In cement mortar",4.2006302000000004E-3,"cum",8,0,{"$f":"+ROUND(C19*G22,2)","v":0}]
[14,"Providing and laying Non Pressure NP-3 class (Medium duty) R.C.C. pipes including collars/spigot jointed with stiff mixture of cement mortar in the proportion of 1:2 (1 cement : 2 fine sand) including testing of joints etc. complete...900 mm dia RCC pipes.",9.3524855200000007E-2,"mtr",15,0,{"$f":"+ROUND(C20*G22,2)","v":0}]
[15,"Not covered in above but covered in  DSR-2016",2.77030199E-2,1,15000,0,{"$f":"+ROUND(C21*G22,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C21)","v":1},"Total amount quoted by bidder",null,null,0]
[null,"IN WORDS",{"$f":"rup(G22)","v":0}]
[]
["Note:","1. GST extra as applicable"]
[null,"2. Bidder has to quote in above unlocked cell (G-22) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"3. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"4.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[null,null,null,null,"(Signature and Seal of  Contractor  )"]