{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Price bid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Price bid","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,11,0,19],[8,0,8,2],[8,3,8,6],[10,1,10,6],[11,1,11,6],[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6]]}
["BHARAT HEAVY ELECTRICALS LIMITED,  JHANSI"]
["FACTORY CIVIL DEPARTMENT"]
["Price bid "]
["NAME OF WORK: Water proofing work for pit of New bogie shop."]
["Tender Number: FCX/TW/24/13"]
["Sr. No","Description ","% Allocation (Item-wise)","Unit "," Qty","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Providing and fixing the packers of diameter minimum 14 mm and length as per requirement of concrete structure. THe packers are to be fixed by making a grid of approximately 2 feet x 2 feet on the effected area. After fixing the packer, injection grouting is to be carried out with Low Viscous Injection Grout though Pressure grouting machine using appropriate pressure. Grouting material is to be injected till the void/cavity inside the RCC is completely filled and packer stops accepting the grouting material further. After fillng all the packer should be removed with the help of hammer and the hole is to be repaired with the help of cement mortar.\nMaterial of Low Viscous injection grouting should be Fosroc Conbextra EP10 LV/Asian Paint Apco Rep LV/Sika SikaDur LV.",{"$f":"375000/375000","v":1},"Per Nozzle ",500,{"$f":"ROUND(G7/E7,4)","v":0},{"$f":"C7*G8","v":0}]
[null,"Total (Excluding GST) (In Rs.)",{"$f":"SUM(C7:C7)","v":1},null,null,null,0]
["In words ",null,null,{"$f":"rup(G8)","v":0}]
[null,"Note -GST extra as applicable"]
[null,"1. Bidder has to quote in above unlocked cell (G-8) only. Item rate shall be calculated automatically. Calculated item rates upto four  decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected."]
[]
[]
[]
[null,null,null,"(Signature and Seal of  Contractor  )"]