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ISO 9001:2008, 14001:2004, 50001:2011 & OHSAS 18000

MAHARATNA COMPANY
	MATERIAL MANAGEMENT (PURCHASE)

                          CENTRAL FOUNDRY FORGE PLANT, BHEL HARDWAR

RANIPUR, HARIDWAR  (INDIA) – 249403

Phone No.+91-1334-281360/285524, FAX No. 225892

e-mail :rajesh.kur@bhel.in; skkwat@bhel.in



REF: Tender Enquiry No: 202001891 (EVENT ID: 48670) due on, at 14:00 PM for Ingot Mould 1700 MM
Acceptance Criteria for 1700 Ingot Mould
Acceptance Criteria for 1700 mm Ingot Mould will be under:

1. Following Documents are required along with supply of Ingot Mould:  

a) Original Manufacturer’s Test Certificate (including Dimensional Report, 

Test of Chemical Analysis, Hardness Report, Heat Treatment/SR cycle etc) in line with CFFP Specification & Drawing of Tender Enquiry.

b)  Third party inspection certificate in line with CFFP specification of Tender 

      Enquiry.
2. Ingot Mould will be used in minimum 3 (Three) heats and performance will be checked for development of any crack/metallic erosion. (This testing will be completed within 60 days from the receipt of material and documents mentioned at Point 1 above)
Acceptance to both the points (1 & 2 as mentioned above) will be one of the qualification criteria for Technical suitability of Participating Vendors.
(Signature of Vendor & Seal)

