{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["price bid "],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"price bid ","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[[16,1,16,6],[14,1,14,6],[15,1,15,6],[0,0,0,6],[3,0,3,6],[1,0,1,6],[2,0,2,6],[4,0,4,2],[4,4,4,6],[12,2,12,6],[11,3,11,5]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["FACTORY CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:-  Misc. fabrication work in BHEL jhansi"]
["Tender Enq No-FCX/TW/22/07"]
["Sl. No.","Description of Work","% Allocation (Item-wise)","Unit ","Quantity ","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"The existing electrical motorized rolling shutter is to be replaced with a mechanical gear box based system by providing and fixing gear box and spring shaft & the interlocking GI rolling strips are to be used from the existing gate. The work includes dismantling of existing gate and installation of appropriate mechanized system using existing GI interlocking strips. All tools and tackles shall be arranged by the contractor. \nSize of the gate -4.00 x7.00 mtr. (Approx.)\n",44.221698113199999,"Job",1,{"$f":"ROUND(G7/E7,2)","v":0},{"$f":"ROUND($G$12*C7%,2)","v":0}]
[2,"One time effective servicing, attending minor repairs during the servicing, greasing for all type of rolling shutters  for all sizes etc., complete as per the specifications and instructions of the Engineer-in-charge. The quoted rate is for the repairs, all adjustments, bolt nut tightening including removing shutters, brackets and other accessories if necessary, re-fixing the shutter in position and all other incidental charges, tools and plants complete ."]
["2.(a)","For gate size upto 30 sqm",23.349056603800001,"Each",9,{"$f":"ROUND(G9/E9,2)","v":0},{"$f":"ROUND($G$12*C9%,2)","v":0}]
["2.(b)","For gate size above 30 sqm up to 50 sqm",22.700471698099999,"Each",7,0,{"$f":"ROUND($G$12*C10%,2)","v":0}]
["2.(c)","For gate size above 50 sqm",9.7287735849000008,"Each",2,0,{"$f":"ROUND($G$12*C11%,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C11)","v":100},"Total amount quoted by bidder"]
[null,"IN WORDS",{"$f":"rup(G12)","v":0}]
[null,"Note -GST extra as applicable"]
[null,"1. Bidder has to quote in above unlocked cell (G-12) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"3.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[]
[null,null,null,"(Signature and Seal of  Contractor  )"]