{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["price bid "],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"price bid ","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[[15,1,15,6],[13,1,13,6],[14,1,14,6],[0,0,0,6],[3,0,3,6],[1,0,1,6],[2,0,2,6],[4,0,4,2],[4,4,4,6],[11,2,11,6],[10,3,10,5]]}
["    BHARAT HEAVY ELECTRICAL LIMITED , JHANSI              "]
["FACTORY CIVIL DEPARTMENT"]
["PRICE BID (JS 146)"]
["Name of work:-  Misc. fabrication work in BHEL jhansi"]
["Tender Enq No-FCX/TW/22/06"]
["Sl. No.","Description of Work","% Allocation (Item-wise)","Unit ","Quantity ","Rate per Unit (in Rs.)","Amount (in Rs.)"]
[1,"Dismantling steel work in built up sections in angles, tees, flats and channels including all gusset plates, bolts, nuts, cutting rivets, welding etc. including dismembering and stacking within 50 metres lead.",7.8066113922999998,"Kg",15000,{"$f":"ROUND(G7/E7,2)","v":0},{"$f":"ROUND($G$11*C7%,2)","v":0}]
[2,"Fabrication and erection of structural steel works at all heights(Maximum height up to 30.0 m) consisting of, railing, clamps, purlins with channels & angles,  M.S. flat, M.S. tubes, supports including all connections as per detailed drawings connected steel works etc. cleats, gusset plates all bolts, nuts, washers ,base plates, anchor bolts etc., as per detailed drawings cutting welding and painting 1 coats of red oxide primer before erection & 2 coats of synthetic enamel paint/Aluminium paint of approved brand & colour after erection complete. Advani made electrodes or other approved make electrodes are to be used. All bolts, nuts, washers, gas, electrodes are in contractor's scope. Fabrication to be done as per I.S. codes of latest revision. (All the materials are in contractor scope except the Structural steel. Structural steel shall be provided by BHEL free of cost.) (Make of paint and primer shall be Asian, Berger, Narolac and Salimar)\n"]
[null,"Only fabrication",36.890276730899998,"Kg",27000,{"$f":"ROUND(G9/E9,2)","v":0},{"$f":"ROUND($G$11*C9%,2)","v":0}]
[null,"Only erection",55.303111876800003,"Kg",27000,{"$f":"ROUND(G10/E10,2)","v":0},{"$f":"ROUND($G$11*C10%,2)","v":0}]
[null,"Total ",{"$f":"SUM(C7:C10)","v":100},"Total amount quoted by bidder"]
[null,"IN WORDS",{"$f":"rup(G11)","v":0}]
[null,"Note -GST extra as applicable"]
[null,"1. Bidder has to quote in above unlocked cell (G-11) only. Item rate shall be calculated automatically. Calculated item rates upto four decimal points may be adjusted w.r.t. gross total amount and it shall be the itemwise final rate for  execution of contract and all other purposes."]
[null,"2. Quoted gross total amount should be considered only if quoted in this excel sheet and print out of this should only be considered for evaluation.  If Price is quoted in any other format other than the Excel Sheet enclosed to the NIT , the offer of the bidder  will be rejected"]
[null,"3.During the execution , the quantity of various items may vary to any extent depending on requirement of work/site and as per discretion of BHEL."]
[]
[]
[null,null,null,"(Signature and Seal of  Contractor  )"]