SEATING

PRODUCT SPECIFICATION SHEET
1) SEAT/BACK ASSEMBLY: The seat and back are made up of 1.2 cm. thick hot-
     pressed plywood, upholstered with fabric upholstery covers and moulded 
     Polyurethane foam. The back foam is designed with contoured lumbar support for 
     extra comfort. The seat has extra thick foam on front edge to give comfort to 
     popliteal area.

SEAT SIZE

         :
           50.5 cm (W) X 52.5 cm (L)
BACK SIZE                      :            50.5 cm (W) x 69.5 cm (H)

2)  POLYURETHANE FOAM: The Polyurethane foam is moulded with density = 45 +/-2 
     kg/m3 and Hardness = 20+/- 2 at 25% compression.

3)  ARMRESTS: The one-piece armrests are injection moulded from black Co-polymer 
     Polypropylene.
ARMREST SIZE                      :            43 cm (L) x 25 cm (H)

4)  CENTER TILT SYNCHRO MECHANISM    : The mechanism is designed with the 
      following features:

      · 3600 revolving type.

      · Upright position locking.

      · Tilt tension adjustment.

      · Seat/back tilting ratio of 1:3 (60 seat tilt/180 back tilt)

5)  PNEUMATIC HEIGHT ADJUSTMENT   : The pneumatic  height adjustment has an 
     adjustment stroke of 12.0 cm.

6)  TELESCOPIC BELLOW ASSEMBLY   : The below is 3 piece telescopic type and 
      Injection moulded in black Polypropylene.

7)  PEDESTAL ASSEMBLY   : The pedestal is injection moulded in black 30% glass-
     filled Nylon and fitted with 5 nos. twin wheel castors. 
     The pedestal is 66.0cm pitch-center dia. (76.0 cm with castors.)

8)  TWIN WHEEL CASTORS: The twin wheel castors are injection moulded in Black 
      Nylon.
9)  Warranty: 2 years replacement warranty against any physical damage due to    manufacturing defects. 

                                                                                                                       Page 1 of 2               

SEATING

PRODUCT SPECIFICATION SHEET
[image: image1.emf]


WIDTH (W)         78.0 CM
DEPTH (D)         78.0 CM

        HEIGHT(H)        102 – 114 CM
       SEAT HEIGHT(SH)  46- 58 CM
       UNSPECIFIED TOL- ± 1.0 CM

Material Code: HY7802161762
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