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PRE QUALIFICATION REQUIREMENT (TECHNICAL)
Titanium Cladded Plate (CS + Ti)
Ref: Titanium Cladded Plate (Carbon Steel plate-ASTM A36/IS2062 GR A/IS2062 E250 Gr BR + ASTM B265 Gr.2 (UNS R50400) as per Spec: TDC: RTS: 003 Rev 01. (Ti 2mm + Carbon Steel 7mm) X Width 2500 mm X Length 6000mm, Quantity=2050 MT.
The  following Pre-Qualification Criteria for participating in the Tender
A: Technical Competence:
(1) ) Manufacturers to confirm all the clauses (1.0 to 12.2) and Drawing No:4-FW-000-00790 Rev00 as called for in the TDC: RTS: 003 Rev 01.
(2) Manufacturers having Mills for Explosion Bonding or hot rolling or combination of Explosion Bonding or hot rolling facilities are only eligible to participate.
(3) ) Manufacturers shall submit valid license certificate for explosion bonding.
B: Financial Information:
(1) Manufacturers Turnover (T/O) shall be 30% of our tender estimation.
(2) Manufacturers Net worth shall be positive.
Necessary supporting documents shall be submitted for meeting each of the above Pre-Qualification Criteria for evaluation of the offers.

BHEL reserves the right to consider/Not-consider the offers based on the evaluation of documents submitted for the above Pre-Qualification Criteria. BHEL also reserves the right to have on-site assessment of the facilities at supplier’s works during the bid evaluation.
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